Project Name:	Kemerton
	Project Code:	KEM	Site ID:	P784	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	AMG ref.: 384450. 6325150. Flat slope
	Date Desc.:	23/05/85	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	115.766666666667	Runoff:	No Data
	Easting/Lat.:	-33.2	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Humus podzol
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Very dark grey (10YR3/1-Dry); ; Sand (Sapric); Single grain grade of structure; Very weak 
	consistence; 
	0.05 - 0.1 m	Dark grey (10YR4/1-Moist); ; Sand (Sapric); Single grain grade of structure; Very weak 
	consistence; 
	0.1 - 0.2 m	Dark grey (10YR4/1-Moist); Grey (10YR5/1-Moist); ; Sand; Single grain grade of structure; Loose 
	consistence; Gradual change to - 
	0.2 - 0.3 m	Grey (10YR5/1-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	0.3 - 0.6 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	0.6 - 1 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	1 - 1.35 m	; Sand; Single grain grade of structure; Loose consistence; 
	1.35 - 1.4 m	; Sand; Single grain grade of structure; Loose consistence; 
	Morphological Notes
	Much fine powdery organic matter between sandgrains
	Water table at 80 cm
	Observation Notes
	B.D. samples, each of 4 bulked cores from following depths: 0-6.8, 27-33, 57-63 cm. Last sample probably useless, because 
	of extreme wetness and proneness to wall collapse.
	Site Notes
	Cattel grazing on annula pastures. Orig. Maleleuca swamp, now cleared. Rushes in wettest areas. Very broad interdune hollow.
	 Siliceous sand of prob. Aeolian origin. Poor external drainage. Intern. Drainage impeded by org. B hor. At 80 cm.

	Project Name:	Kemerton
	Project Code:	KEM	Site ID:	P784	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.1A	0.04A	4K	0.58	0.04	0.07	8.7D
	0.05 - 0.1	4.9A	0.03A	1.2K	0.05	0.01	0.03	8.8D
	0.1 - 0.2	4.7A	0.04A	1.4K	0.1	0.02	0.31	4.9D
	0.2 - 0.3	4.6A	0.02A	0.14K	0	0	0
	0.3 - 0.6	4.5A	0.02A	0.03K	0	0.01	0
	0.6 - 1	4.9A	0.04A	0.02K	0	0	0
	1 - 1.35	5.1A	0.03A	0K	0.1	0	0
	1.35 - 1.4	5A	0.04A	0K	0.25	0	0.08
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	3.8D	4.4D	54F	0.185B	86D	3
	0.05 - 0.1	1.63D	1.8D	16F	0.064B	88D	4
	0.1 - 0.2	0.923D	1.5D	12F	0.066B	87D	7
	0.2 - 0.3	0.372D	1.1D	7.2F	0.015B	92D	6	2	1
	0.3 - 0.6	0.176D	2.2D	7.4F	0.013B	89D	9	1	1
	0.6 - 1	0.121D	2.3D	9.7F	0.009B
	1 - 1.35	0.306D	3.7D	11F	0.02B
	1.35 - 1.4	1.56D	7.3D	12F	0.039B	84D	10
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 1
	1 - 1.35
	1.35 - 1.4

	Project Name:	Kemerton
	Project Code:	KEM	Site ID:	P784	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	13A1_AL	Oxalate-extractable aluminium
	13A1_FE	Oxalate-extractable iron
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9E	Available P (mg/kg) - Bray P
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance