Project Name:	KOJ
	Project Code:	KOJ	Site ID:	P430	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	M.J. Mulcahy	Locality:
	Date Desc.:	15/08/60	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	Runoff:	Rapid
	Easting/Lat.:	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediplain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Pediment	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Magnesic-Natric Red Kurosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; ; FragmentLoose consistence; 0-2%, 
	Substrate material, coarse fragments; Sharp change to - 
	0.1 - 0.33 m	Light reddish brown (5YR6/3-Moist); , 5YR51, 2-10% ; , 10YR56, 2-10% ; Clay loam; Diffuse 
	change to - 
	0.33 - 0.61 m	Light reddish brown (5YR6/3-Moist); , 10YR56; , 5YR81; Medium clay; Moderate grade of 
	structure, Subangular blocky; Weak consistence; Diffuse change to - 
	0.61 - 1.02 m	Light reddish brown (5YR6/3-Moist); , 5YR81; , 10YR56; Medium clay; Moderate grade of 
	structure, Subangular blocky; Weak consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	KOJONUP

	Project Name:	KOJ
	Project Code:	KOJ	Site ID:	P430	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.2A	 0.268A	 7.1K	 2.7	 0.1	 0.45
	0.1 - 0.33	5.5A	 0.774A	 0.8K	 3.7	 0.1	 0.43
	0.33 - 0.61	5.1A	 1.07A	 0.3K	 4.6	 0.06	 0.87
	0.61 - 1.02	5.1A	 1.37A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 4.89D	 0.01D	 0.167B	 36D	 32	 10	 11
	0.1 - 0.33	 2.1D	 0.003D	 0.017B	 22D	 13	 15	 47
	0.33 - 0.61	 3.4D	 0.003D	 0.014B	 14D	 5	 12	 62
	0.61 - 1.02	 2.5D	 0.002D	 19D	 6	 16	 56
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.1 - 0.33
	0.33 - 0.61
	0.61 - 1.02

	Project Name:	KOJ
	Project Code:	KOJ	Site ID:	P430	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance