Project Name:	MAN
	Project Code:	MAN	Site ID:	P333	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	North base line 5.7KM west of South Stirlings Road:
	Date Desc.:	26/03/57	Elevation:	No Data
	Map Ref.:	Sheet No. : 2528   1:100000	Rainfall:	0
	Northing/Long.:	118.145	Runoff:	No Data
	Easting/Lat.:	-34.6188888888889	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Yellow Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree mallee, , . *Species includes - Eucalyptus tetrodonta
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Light brownish grey (10YR6/2-Moist); ; Fine sand; Clear, Smooth change to - 
	0.05 - 0.1 m	Light olive grey (5Y6/2-Moist); ; Fine sand; 2-10%, fine gravelly, 2-6mm, Substrate material, 
	coarse fragments; Gradual change to - 
	0.1 - 0.25 m	Light olive grey (5Y6/2-Moist); ; Fine sand; 20-50%, fine gravelly, 2-6mm, Substrate material, 
	coarse fragments; Clear, Irregular change to - 
	0.25 - 0.61 m	Brownish yellow (10YR6/8-Moist); , 10YR53; Fine sandy medium clay; , Prismatic; Weak 
	consistence; 
	0.61 - 0.91 m	Light grey (10YR7/1-Moist); , 10YR78; , 5YR44; Fine sandy medium clay; Weak consistence; 
	0.91 - 1.22 m	Grey (10YR6/1-Moist); , 10YR66; Fine sandy medium clay; 
	Morphological Notes
	Observation Notes
	5-25CM AL GV IS FERRUGINOUS                                                                                             
	Site Notes

	Project Name:	MAN
	Project Code:	MAN	Site ID:	P333	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6A	 0.03A	 1.5K	 0.9	 0.07	 0.05	 2.4E	 4.9B
	0.05 - 0.1	6.9A	 0.036A	 0.3K	 0.7	 0.04	 0.03	 1.8E	 2.9B
	0.1 - 0.25	6.4A	 0.012A
	0.25 - 0.61	6.6A	 0.054A	 1.7K	 5.9	 0.44	 1.2
	0.61 - 0.91	7.5A	 0.093A	 1.6K	 6.4	 0.42	 1.6
	0.91 - 1.22	7.8A	 0.381A	 2.1K	 0.9	 0.6	 4.8
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.002D	 0.046B	 32D	 62	 1	 2
	0.05 - 0.1	 33D	 63	 1	 2
	0.1 - 0.25
	0.25 - 0.61	 17D	 39	<1	 43
	0.61 - 0.91	 18D	 47	<1	 33
	0.91 - 1.22	 0.001D	 15D	 48	<1	 36
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.25
	0.25 - 0.61
	0.61 - 0.91
	0.91 - 1.22

	Project Name:	MAN
	Project Code:	MAN	Site ID:	P333	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance