Project Name:	MAP
	Project Code:	MAP	Site ID:	P683	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	27KM W.S.W. of Manjimup + 9.4KM S.W. of One-
	Tree Bridge : in 50M X 50Mplot 0.3KM N.W. of Pine 
	Creek Road:
	Date Desc.:	16/12/76	Elevation:	 160 metres
	Map Ref.:	Sheet No. : 2029   1:100000	Rainfall:	1250
	Northing/Long.:	115.85	Runoff:	Rapid
	Easting/Lat.:	-34.2666666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.15
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Dry; Loose 
	consistence; 50-90%, fine gravelly, 2-6mm, Substrate material, coarse fragments; Common, 
	fine (1-2mm) roots; 
	A21	0.05 - 0.1 m	Yellowish red (5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Moist; Very weak 
	consistence; 50-90%, fine gravelly, 2-6mm, Substrate material, coarse fragments; Common, 
	fine (1-2mm) roots; 
	A22	0.1 - 0.2 m	Yellowish red (5YR4/8-Moist); ; Sandy loam (Heavy); Massive grade of structure; Moist; Very 
	weak consistence; 50-90%, fine gravelly, 2-6mm, Substrate material, coarse fragments; 
	Common, fine (1-2mm) roots; 
	A23	0.2 - 0.3 m	Yellowish red (5YR4/8-Moist); ; Sandy loam (Heavy); Massive grade of structure; Moist; Very 
	weak consistence; 50-90%, fine gravelly, 2-6mm, angular, Gravel, coarse fragments; Few, 
	medium (2-5mm) roots; 
	A24	0.3 - 0.6 m	Yellowish red (5YR4/8-Moist); ; Clay loam; Massive grade of structure; Moist; Weak 
	consistence; 2-10%, medium gravelly, 6-20mm, angular, Gravel, coarse fragments; Few, 
	medium (2-5mm) roots; 
	B	0.6 - 0.75 m	Red (2.5YR4/8-Moist); ; Light clay; Massive grade of structure; Moist; Very weak consistence; 2-
	10%, medium gravelly, 6-20mm, angular, Quartz, coarse fragments; 
	BC	0.75 - 0.9 m	Red (2.5YR4/8-Moist); , 5YR58; Medium clay; Massive grade of structure; Moist; Very weak 
	consistence; 2-10%, fine gravelly, 2-6mm, Gravel, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-20CM AL GV IS FERRUGINOUS AND A FEW ANGULAR SILICA GRAVEL <30MM ALSO:LAYERS RE NUMBERED 15/10/92  
	                    
	Site Notes

	Project Name:	MAP
	Project Code:	MAP	Site ID:	P683	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.4A	 0.054A
	0.05 - 0.1	6.9A	 0.024A	 6.17K	 1.24	 0.3	 0.11	 7.8B
	0.1 - 0.2	7A	 0.018A	 5.83K	 1.04	 0.27	 0.08	 7.2B
	0.2 - 0.3	7A	 0.015A	 5.45K	 0.86	 0.35	 0.08	 6.7B
	0.3 - 0.6	6.8A	 0.009A	 2.47K	 0.44	 0.31	 0.04	 3.3B
	0.6 - 0.75	6.8A	 0.009A	 1.55K	 0.19	 0.19	 0.09	 2B
	0.75 - 0.9	6.7A	 0.006A	 1.49K	 0.12	 0.16	 0.03	 1.8B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 12D	 0.015D	 0.256B	 0.115A
	 0.028A
	0.05 - 0.1	 3.82D	 6.4D	 0.012D	 0.19B	 0.116A
	 0.021A
	0.1 - 0.2	 2.63D	 6.9D	 0.011D	 0.153B	 0.11A
	 0.012A
	0.2 - 0.3	 2.08D	 4.1D	 0.01D	 0.121B	 0.118A
	 0.022A
	0.3 - 0.6	 0.82D	 4.6D	 0.007D	 0.047B	 0.12A
	 0.016A
	0.6 - 0.75	 0.61D	 2.8D	 0.006D	 0.032B	 0.07A
	 0.012A
	0.75 - 0.9	 0.82D	 2.2D	 0.007D	 0.032B	 0.038A
	 0.011A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.75
	0.75 - 0.9

	Project Name:	MAP
	Project Code:	MAP	Site ID:	P683	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_CU	Ammonium bicarbonate/EDTA - extractable copper
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF