Project Name:	MAP
	Project Code:	MAP	Site ID:	P689	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	25KM west of Manjimup and 8.4KM S.W. of One-Tree
	 Bridge: adjacent to west side of Pine Creek Road:
	Date Desc.:	14/12/76	Elevation:	 150 metres
	Map Ref.:	Sheet No. : 2029   1:100000	Rainfall:	1250
	Northing/Long.:	115.333333	Runoff:	Rapid
	Easting/Lat.:	-34.25	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.15
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Moist; Very weak 
	consistence; 50-90%, fine gravelly, 2-6mm, rounded, Substrate material, coarse fragments; 
	Common, fine (1-2mm) roots; 
	A12	0.05 - 0.1 m	Reddish brown (5YR4/4-Moist); ; Sandy loam (Heavy); Massive grade of structure; Moist; Very 
	weak consistence; 50-90%, fine gravelly, 2-6mm, rounded, Substrate material, coarse 
	fragments; Common, fine (1-2mm) roots; 
	0.1 - 0.2 m	Yellowish red (5YR4/6-Moist); ; Sandy loam (Heavy); Massive grade of structure; Very weak 
	consistence; 50-90%, fine gravelly, 2-6mm, rounded, Substrate material, coarse fragments; 
	Common, fine (1-2mm) roots; 
	0.2 - 0.3 m	Yellowish red (5YR4/8-Moist); ; Sandy clay loam; Massive grade of structure; Very weak 
	consistence; 50-90%, fine gravelly, 2-6mm, rounded, Substrate material, coarse fragments; 
	Few, coarse (>5mm) roots; 
	0.3 - 0.6 m	Red (2.5YR4/8-Moist); ; Clay loam (Heavy); Massive grade of structure; Very weak consistence; 
	10-20%, fine gravelly, 2-6mm, rounded, Substrate material, coarse fragments; Few, fine (1-2mm)
	 roots; 
	0.6 - 0.8 m	Yellowish red (5YR4/8-Moist); ; Light clay; Massive grade of structure; Weak consistence; 50-
	90%, coarse gravelly, 20-60mm, angular, Quartzite, coarse fragments; 
	0.8 - 0.9 m	Strong brown (7.5YR5/6-Moist); ; Medium clay; Massive grade of structure; Weak consistence; 
	50-90%, coarse gravelly, 20-60mm, subrounded, Substrate material, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-60CM AL GV IS FERRUGINOUS: 80-90CM AL GV IS W'D ROCK: 0-10CM <10% <10MM ANGULAR QZ ALSO: 30-90CM 
	ANGULAR QZ ALSO:     LAYERS RE NUMBERED 15/10/92
	Site Notes

	Project Name:	MAP
	Project Code:	MAP	Site ID:	P689	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.3A	 0.092A	 21.3K	 1.56	 0.52	 0.23	 23.6B
	0.05 - 0.1	6.9A	 0.021A	 9.02K	 1.34	 0.29	 0.19	 10.8B
	0.1 - 0.2	6.5A	 0.015A	 4.14K	 0.78	 0.2	 0.12	 5.2B
	0.2 - 0.3	6.5A	 0.009A	 2.85K	 0.67	 0.17	 0.1	 3.8B
	0.3 - 0.6	6.4A	 0.006A	 1.28K	 0.45	 0.16	 0.06	 2B
	0.6 - 0.8	6.5A	 0.006A	 0.92K	 0.3	 0.3	 0.05	 1.6B
	0.8 - 0.9	6.5A	 0.006A	 0.69K	 0.23	 0.33	 0.12	 1.4B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 7.4D	 7.4D	 0.013D	 0.285B	 0.184A	 51
	 0.025A
	0.05 - 0.1	 5.48D	 5.5D	 0.009D	 0.224B	 0.159A	 60
	 0.024A
	0.1 - 0.2	 3.38D	 5.9D	 0.01D	 0.16B	 0.164A	 47
	 0.021A
	0.2 - 0.3	 2.04D	 4.7D	 0.006D	 0.092B	 0.167A	 46
	 0.017A
	0.3 - 0.6	 1.26D	 4.4D	 0.003D	 0.04B	 0.142A	 42
	 0.014A
	0.6 - 0.8	 0.39D	 3.6D	 0.003D	 0.021B	 0.066A	 45
	 0.012A
	0.8 - 0.9	 0.29D	 4.3D	 0.006D	 0.017B	 0.05A	 54
	 0.014A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	0.8 - 0.9

	Project Name:	MAP
	Project Code:	MAP	Site ID:	P689	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_CU	Ammonium bicarbonate/EDTA - extractable copper
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	P10_GRAV	Gravel (%)
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF