Project Name:	NER
	Project Code:	NER	Site ID:	P382	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	Wagin L.A. 388/80: 24 chains south east of P379: 
	south east side of Lake Camm:
	Date Desc.:	17/07/58	Elevation:	No Data
	Map Ref.:	Rainfall:	360
	Northing/Long.:	119.583056	Runoff:	Very rapid
	Easting/Lat.:	-32.985	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediplain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Hypercalcic Yellow Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solonized brown 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0.08 - 0.15 m	Greyish brown (10YR5/2-Moist); ; Sand (Fibric); 
	A2	0.2 - 0.25 m	Light brownish grey (2.5Y6/2-Moist); ; Sand; 
	B	0.25 - 0.36 m	Light yellowish brown (10YR6/4-Moist); ; Sandy medium clay; Irregular change to - 
	0.51 - 0.66 m	Yellowish brown (10YR5/4-Moist); ; Sandy medium clay; Weak consistence; 10-20%, 
	Limestone, coarse fragments; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	WAGIN L.A.

	Project Name:	NER
	Project Code:	NER	Site ID:	P382	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.08 - 0.15	8.3A	 0.063A
	0.25 - 0.36	9.3A	 0.3A
	0.51 - 0.66	9.4A	 0.75A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.08 - 0.15	<1A	 53D	 36	 4	 7
	0.25 - 0.36	<1A	 40D	 18	 3	 40
	0.51 - 0.66	 1A	 28D	 14	 7	 47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.08 - 0.15
	0.25 - 0.36
	0.51 - 0.66

	Project Name:	NER
	Project Code:	NER	Site ID:	P382	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance