Project Name:	NST
	Project Code:	NST	Site ID:	P15	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	R. Hare	Locality:	5.7KM south of Borden:middle of east boundary of 
	location 2923:
	Date Desc.:	01/02/49	Elevation:	No Data
	Map Ref.:	Sheet No. : 2529   1:100000	Rainfall:	0
	Northing/Long.:	118.26	Runoff:	Rapid
	Easting/Lat.:	-34.1202777777778	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gabbro 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mesonatric Brown Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Loam; 
	0.05 - 0.18 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; 
	0.18 - 0.46 m	Dark brown (10YR3/3-Moist); ; Medium clay; 
	0.46 - 0.76 m	Brown (10YR4/3-Moist); , 10YR62; , 5G62; Light clay; Few (2 - 10 %), Calcareous, , Concretions;
	Morphological Notes
	Observation Notes
	>30CM SPECKLED DECOMPOSED GABBRO:                                                                                       
	Site Notes
	PLANTAGENET LD

	Project Name:	NST
	Project Code:	NST	Site ID:	P15	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.6A	 0.116A	 15.1K	 8.8	 1.37	 0.57	 7.8E	 32.6B
	0.05 - 0.18	9A	 0.848A	 13K	 18.7	 1.02	 6.69	 39.4B
	0.18 - 0.46	9.2A	 1.28A
	0.46 - 0.76	9.4A	 1.88A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.02A	 3.95D	 0.026D	 0.234B	 5	 25D	 35	 14	 20
	0.05 - 0.18	 0.29A	 1.35D	 0.017D	 0.058B	 5	 23D	 24	 8	 40
	0.18 - 0.46	 1.87A	 3	 20D	 23	 7	 46
	0.46 - 0.76	 21.1A	 2	 12D	 16	 10	 39
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.18
	0.18 - 0.46
	0.46 - 0.76

	Project Name:	NST
	Project Code:	NST	Site ID:	P15	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance