Project Name:	PIN
	Project Code:	PIN	Site ID:	P356	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	CG.443 east side of road:
	Date Desc.:	11/10/57	Elevation:	No Data
	Map Ref.:	Rainfall:	940
	Northing/Long.:	115.8161111	Runoff:	Rapid
	Easting/Lat.:	-32.78	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Grey Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.15 m	Greyish brown (10YR5/2-Moist); ; Loamy sand; 50-90%, Substrate material, coarse fragments; 
	B	0.46 - 0.61 m	Light olive grey (5Y6/2-Moist); , 10YR56; Sandy medium clay; Common (10 - 20 %), Ferruginous,
	 , Concretions; 
	1.22 - 1.37 m	Light olive grey (5Y6/2-Moist); , 10YR56; Sandy medium clay; Few (2 - 10 %), Ferruginous, , 
	Concretions; 
	1.98 - 2.13 m	Light grey (5Y7/1-Moist); , 5YR44; , 10YR56; Sandy medium clay; 
	CDr	3.05 - 3.35 m	Light grey (5Y7/1-Moist); , 10YR66, 2-10% ; , 10YR52, 2-10% ; Clayey sand; Very many (50 - 100 
	%), Ferruginous, , Concretions; 
	Morphological Notes
	Observation Notes
	0-15CM AL GV IS FERRUGINOUS:122-137CM MOTTLES SHOW VERTICAL STRUCTURE:305-335CM L. AMTS OF HEAVY 
	MINERALS:              
	Site Notes
	MURRAY

	Project Name:	PIN
	Project Code:	PIN	Site ID:	P356	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.3A	 0.057A	 1K	 1	 0.03	 0.16	 5.3E	 7.7B
	0.46 - 0.61	6.2A	 0.045A	 1.5K	 2.6	 0.16	 0.14	 5.2E	 9.6B
	1.22 - 1.37	5.4A	 0.14A
	1.98 - 2.13	4.9A	 0.095A
	3.05 - 3.35	4.2A	 0.214A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 0.93D	 0.005D	 0.059B	 60D	 26	 2	 11
	0.46 - 0.61	 0.006D	 0.016B	 55D	 24	 1	 20
	1.22 - 1.37
	1.98 - 2.13
	3.05 - 3.35	 0.002D
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.46 - 0.61
	1.22 - 1.37
	1.98 - 2.13
	3.05 - 3.35

	Project Name:	PIN
	Project Code:	PIN	Site ID:	P356	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance