Project Name:	SOU
	Project Code:	SOU	Site ID:	P718	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	Corner of Deeside Coast Road and Middleton 
	Road:crest of hill on broadupland:
	Date Desc.:	01/11/82	Elevation:	No Data
	Map Ref.:	Sheet No. : 2128   1:100000	Rainfall:	0
	Northing/Long.:	116.316666666667	Runoff:	No Data
	Easting/Lat.:	-34.5833333333334	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Magnesic Brown Kurosol     	Principal Profile Form:	Dy5.61
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:
	Mid Strata - , , Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; 0-2%, Quartz, coarse 
	fragments; 
	0.05 - 0.15 m	Grey (10YR5/1-Moist); ; Sand; Single grain grade of structure; 2-10%, Quartz, coarse fragments; 
	0.15 - 0.3 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; 2-10%, Quartz, coarse 
	fragments; 
	0.3 - 0.5 m	Yellowish brown (10YR5/6-Moist); , 10YR61; Sandy medium clay; Massive grade of structure; 2-
	10%, Quartz, coarse fragments; 
	0.5 - 0.7 m	Yellowish brown (10YR5/6-Moist); , 5Y62; Medium clay; Massive grade of structure; 2-10%, 
	Quartz, coarse fragments; 
	0.7 - 0.9 m	Yellowish brown (10YR5/5-Moist); , 5Y52; , 10YR51; Medium clay; Massive grade of structure; 0-
	2%, Quartz, coarse fragments; 
	0.9 - 1 m	Brownish yellow (10YR6/6-Moist); , 10YR71; Medium clay; Massive grade of structure; 0-2%, 
	Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	THESE SOILS SOMETIMES HAVE FERRUGINOUS-ORGANIC PAN JUST ABOVE CLAY HORIZON:                                           
	  
	Site Notes

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P718	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.2A	 0.003A	 0.4K	 0.56	 0.09	 0.1
	0.15 - 0.3	4.6A	 0.003A
	0.3 - 0.5	5.1A	 0.003A	 0.01K	 0.02	 0.03	 0.03
	0.5 - 0.7	5.1A	 0.003A	 0.02K	 0.37	 0.03	 0.1
	0.9 - 1	5.2A	 0.003A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 3.3D	 46D	 47	 3	 3
	0.15 - 0.3
	0.3 - 0.5	 22D	 25	 11	 40
	0.5 - 0.7
	0.9 - 1	 19D	 9	 6	 66
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.15 - 0.3
	0.3 - 0.5
	0.5 - 0.7
	0.9 - 1

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P718	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance