Project Name:	SOU
	Project Code:	SOU	Site ID:	P732	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	Weld Road 7.2KM from Thomson Road:
	Date Desc.:	02/11/82	Elevation:	No Data
	Map Ref.:	Sheet No. : 2228   1:100000	Rainfall:	0
	Northing/Long.:	116.616666666667	Runoff:	No Data
	Easting/Lat.:	-34.7166666666667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Dystrophic Red Kandosol     	Principal Profile Form:	Gn2.12
	ASC Confidence:	Great Soil Group:	Red earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark reddish brown (5YR3/4-Moist); ; Loam; 2-10%, Substrate material, coarse fragments; 
	0.05 - 0.1 m	Reddish brown (5YR4/4-Moist); ; Loam (Heavy); 2-10%, Substrate material, coarse fragments; 
	0.1 - 0.2 m	Red (2.5YR4/6-Moist); ; Clay loam; 2-10%, Substrate material, coarse fragments; 
	0.3 - 0.4 m	Red (2.5YR4/8-Moist); ; Light clay; 20-50%, Substrate material, coarse fragments; 
	0.4 - 0.6 m	Red (2.5YR4/8-Moist); ; Medium clay; 10-20%, Substrate material, coarse fragments; 
	0.6 - 0.8 m	Red (2.5YR4/8-Moist); ; Medium clay; 
	0.8 - 1 m	Red (2.5YR4/8-Moist); , 10YR78; Medium clay; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P732	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.1A	 0.012A	 9.9K	 1.29	 0.34	 0.16
	0.05 - 0.1	7.2A	 0.009A
	0.1 - 0.2	7.1A	 0.006A	 2K	 0.81	 0.17	 0.21
	0.3 - 0.4	7.2A	 0.006A
	0.4 - 0.6	7.1A	 0.003A
	0.8 - 1	6.7A	 0.003A	 1.16K	 0.38	 0.23	 0.17
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 4.8D	 47D	 36	 9	 5
	0.05 - 0.1
	0.1 - 0.2	 44D	 38	 9	 8
	0.3 - 0.4
	0.4 - 0.6
	0.8 - 1	 8D	 26	 24	 46
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.3 - 0.4
	0.4 - 0.6
	0.8 - 1

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P732	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance