Project Name:	SOU
	Project Code:	SOU	Site ID:	P761	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	Junction of South Coast Highway and Marbellup 
	Road:
	Date Desc.:	05/11/82	Elevation:	No Data
	Map Ref.:	Sheet No. : 2428   1:100000	Rainfall:	0
	Northing/Long.:	117.716666666667	Runoff:	No Data
	Easting/Lat.:	-34.9833333333333	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Flood plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Mottled-Hypernatric Grey Sodosol     	Principal Profile Form:	Dy3.81
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:	Low Strata - Sedge, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Very dark grey (2.5Y3/0-Moist); ; Fine sandy loam; 
	0.05 - 0.1 m	Dark grey (2.5Y4/0-Moist); ; Loamy fine sand; 
	0.1 - 0.15 m	Grey (2.5Y5/0-Moist); ; Fine sand; 
	0.15 - 0.25 m	Light grey (2.5Y7/2-Moist); ; Fine sand; 
	0.25 - 0.4 m	Brown (7.5YR5/2-Moist); ; Fine sand; Few (2 - 10 %), Ferruginous, , Concretions; 
	0.4 - 0.6 m	Light brownish grey (2.5Y6/2-Moist); , 2.5Y84; , 5Y56; Fine sandy medium clay; Massive grade 
	of structure; 
	0.6 - 0.8 m	Light brownish grey (2.5Y6/2-Moist); , 2.5Y86; Fine sandy medium clay; Massive grade of 
	structure; 
	Morphological Notes
	Observation Notes
	10-15CM FINE SPIKULES IN SAND (MICROSCOPIC):                                                                            
	Site Notes

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P761	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.2A	 0.027A	 0.29K	 0.62	 0.05	 0.51
	0.05 - 0.1	5.2A	 0.009A	 0.11K	 0.33	 0.04	 0.24
	0.15 - 0.25	5.6A	 0.003A
	0.4 - 0.6	6.5A	 0.051A	 0.42K	 2.9	 0.03	 1.59
	0.6 - 0.8	6.1A	 0.083A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 2.15D
	0.05 - 0.1
	0.15 - 0.25
	0.4 - 0.6	 27D	 54	 4	 15
	0.6 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.15 - 0.25
	0.4 - 0.6
	0.6 - 0.8

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P761	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance