Project Name:	SOU
	Project Code:	SOU	Site ID:	P764	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	0.25KM north of west end of Wambellup Road: (north 
	east of Wambellup swamp):
	Date Desc.:	05/11/82	Elevation:	No Data
	Map Ref.:	Sheet No. : 2328   1:100000	Rainfall:	0
	Northing/Long.:	117.466666666667	Runoff:	No Data
	Easting/Lat.:	-34.5166666666667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Covered plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Swamp	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Dermosolic Oxyaquic Hydrosol     	Principal Profile Form:	Uf6.13
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark grey (10YR4/1-Moist); ; Silty light clay; Weak grade of structure, 10-20 mm, Angular blocky; 
	Moderately plastic; Normal plasticity; 
	0.05 - 0.1 m	Light brownish grey (10YR6/2-Moist); , 10YR51; Medium clay; Weak grade of structure, 10-20 
	mm, Angular blocky; Moderately plastic; Normal plasticity; 
	0.1 - 0.2 m	Light brownish grey (10YR6/2-Moist); , 10YR51; Medium clay; Weak grade of structure, 10-20 
	mm, Angular blocky; Moderately plastic; Normal plasticity; 
	0.3 - 0.4 m	Pale brown (10YR6/3-Moist); ; Medium clay; , Prismatic; Moderately plastic; Normal plasticity; 
	0.5 - 0.6 m	Pale brown (10YR6/3-Moist); ; Medium clay; , Prismatic; Moderately plastic; Normal plasticity; 
	0.7 - 0.8 m	Pale brown (10YR6/3-Moist); ; Medium clay (Light); , Prismatic; Moderately plastic; Normal 
	plasticity; 
	0.9 - 1 m	Very pale brown (10YR7/3-Moist); ; Medium clay; , Prismatic; Moderately plastic; Normal 
	plasticity; 
	1 - 1.1 m	Very pale brown (10YR7/3-Moist); ; Medium clay; , Prismatic; Moderately plastic; Normal 
	plasticity; 
	Morphological Notes
	Observation Notes
	Site Notes
	WAMBELLUP SWP

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P764	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.3A	 0.708A	 3.5K	 14.3	 0.24	 6
	0.1 - 0.2	7.4A	 0.438A	 2.42K	 18.3	 0.23	 6.5
	0.5 - 0.6	7.3A	 0.56A
	0.9 - 1	7.5A	 0.426A	 2.21K	 17.9	 0.13	 6
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 2.5D	 31D	 37	 6	 22
	0.1 - 0.2	 32D	 32	 2	 35
	0.5 - 0.6
	0.9 - 1	 33D	 35	 1	 33
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.1 - 0.2
	0.5 - 0.6
	0.9 - 1

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P764	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance