Project Name:	SOU
	Project Code:	SOU	Site ID:	P768	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	H.M. Churchwood	Locality:	Sturdee Road 1.7KM east of Quangellup Road (east 
	of `Yassanville' - farm to north):
	Date Desc.:	05/11/82	Elevation:	No Data
	Map Ref.:	Sheet No. : 2428   1:100000	Rainfall:	0
	Northing/Long.:	117.516666666667	Runoff:	No Data
	Easting/Lat.:	-34.5333333333333	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Plain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Brown Kandosol     	Principal Profile Form:	Gn2.45
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Massive grade of structure; Weak consistence; 2-10%, 
	Substrate material, coarse fragments; 
	0.05 - 0.1 m	Brown (10YR4/3-Moist); ; Sandy loam; Massive grade of structure; Weak consistence; 20-50%, 
	Substrate material, coarse fragments; 
	0.1 - 0.2 m	Yellowish brown (10YR5/4-Moist); ; Sandy loam; Massive grade of structure; Very weak 
	consistence; 50-90%, Substrate material, coarse fragments; 
	0.3 - 0.4 m	Yellowish brown (10YR5/8-Moist); ; Sandy clay loam; Massive grade of structure; Weak 
	consistence; 50-90%, Substrate material, coarse fragments; 
	0.4 - 0.5 m	Yellowish brown (10YR5/8-Moist); ; Light clay; Weak consistence; 20-50%, Substrate material, 
	coarse fragments; 
	0.5 - 0.6 m	Yellowish brown (10YR5/8-Moist); ; Light clay; 20-50%, Substrate material, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-60CM COARSE FRACTION FERRUGINISED:40-50CM SPIKULES PRESENT (MICROSCOPIC):>60CM FERRUGINISED GV 
	(VERY COARSE):         
	Site Notes
	YASSANVILLE

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P768	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.1A	 0.015A	 8K	 4.1	 0.92	 0.79
	0.05 - 0.1	6.4A	 0.009A	 6.1K	 2.9	 0.93	 0.63
	0.3 - 0.4	6.7A	 0.003A
	0.5 - 0.6	6.7A	 0.006A	 1.69K	 2.58	 0.05	 0.33
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 11D
	0.05 - 0.1
	0.3 - 0.4
	0.5 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.3 - 0.4
	0.5 - 0.6

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P768	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method