Project Name:	SOU
	Project Code:	SOU	Site ID:	P774	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	Mandalay Beach Road 0.5KM west from South-
	Western Highway:
	Date Desc.:	01/11/82	Elevation:	No Data
	Map Ref.:	Sheet No. : 2228   1:100000	Rainfall:	0
	Northing/Long.:	116.6	Runoff:	No Data
	Easting/Lat.:	-34.9666666666667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Calcareous sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Dunefield
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Bleached-Leptic Tenosol     	Principal Profile Form:	Uc2.21
	ASC Confidence:	Great Soil Group:	Podzol
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Shrub, 0.51-1m, Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark grey (10YR4/1-Moist); ; Sand; 
	0.1 - 0.4 m	Light grey (10YR7/2-Moist); ; Sand; 
	0.4 - 0.8 m	Brownish yellow (10YR6/6-Moist); ; Sand; 
	0.8 - 0.9 m	Dark yellowish brown (10YR4/4-Moist); ; Sand; 
	0.9 - 1.4 m	Light yellowish brown (10YR6/4-Moist); ; Sand; 
	1.4 - 1.7 m	Very pale brown (10YR7/3-Moist); ; Sand; Few (2 - 10 %), , , Concretions; 
	1.7 - 2 m	Light grey (10YR7/2-Moist); ; Sand; 
	Morphological Notes
	Observation Notes
	140-200CM CALCAREOUS SAND:                                                                                              
	Site Notes
	WALPOLE

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P774	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1A
	0.1 - 0.4	6A
	0.4 - 0.8	5.6A
	0.8 - 0.9	5.8A
	0.9 - 1.4	6A
	1.4 - 1.7	8.8A
	1.7 - 2	9.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0A
	0.1 - 0.4	 0A
	0.4 - 0.8	 0A
	0.8 - 0.9	 0A
	0.9 - 1.4	 0A
	1.4 - 1.7	 20A
	1.7 - 2	 26A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.4
	0.4 - 0.8
	0.8 - 0.9
	0.9 - 1.4
	1.4 - 1.7
	1.7 - 2

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P774	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	12_HF_FE	Total element - Fe(%) - HF/HClO4 Digest
	19A1	Carbonates - rapid titration
	4A1	pH of 1:5 soil/water suspension