Project Name:	SWV
	Project Code:	SWV	Site ID:	P166	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	L.W. Pym	Locality:	70 chains east of railway on north boundary 1 chain 
	south of north bounary:
	Date Desc.:	27/04/53	Elevation:	 8 metres
	Map Ref.:	Sheet No. : 2134   1:100000	Rainfall:	0
	Northing/Long.:	116.039722222222	Runoff:	Slow
	Easting/Lat.:	-31.7880555555556	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Alluvial plain
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Backplain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Grey Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Alluvial soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.04 m	Dark greyish brown (10YR4/2-Moist); ; Loam (Fibric); Dry; Weak consistence; Diffuse, Smooth 
	change to - 
	A2	0.04 - 0.3 m	Greyish brown (10YR5/2-Moist); , 7.5YR66, 2-10% ; , 2-10% ; Loam; Moist; Weak consistence; 
	Diffuse, Smooth change to - 
	A3	0.3 - 0.63 m	Dark greyish brown (10YR4/2-Moist); , 10YR33; Loam; Moist; Weak consistence; Diffuse, 
	Smooth change to - 
	D	0.63 - 1.19 m	Dark greyish brown (10YR4/2-Moist); ; Fine sand (Heavy); Moist; Weak consistence; 
	Morphological Notes
	Observation Notes
	0-63CM MICACEOUS LOAM:>157CM STRONG BROWN SCLFS + WITH LIGHT BROWN MOTTLE:                                              
	Site Notes
	SOUTH-WEST LD

	Project Name:	SWV
	Project Code:	SWV	Site ID:	P166	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	6.4A	 0.298A
	0.04 - 0.3	6.1A	 0.09A	 10.7K	 7.4	 0.47	 0.38	 14.6E	 33.6B
	0.3 - 0.63	6.5A	 0.042A
	0.63 - 1.19	7A	 0.057A	 3.7K	 3.3	 0.05	 0.5	 3.4E	 10.9B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 6.84D	 0.062D	 0.44B	<1	 3D	 44	 28	 20
	0.04 - 0.3	 0.25B	 2D	 46	 29	 23
	0.3 - 0.63
	0.63 - 1.19	 0.013D	 0.044B	 18	 17D	 57	 9	 15
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.3
	0.3 - 0.63
	0.63 - 1.19

	Project Name:	SWV
	Project Code:	SWV	Site ID:	P166	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance