Project Name:	SWV
	Project Code:	SWV	Site ID:	P176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	L.W. Pym	Locality:	On roadside 2.5chains south east from north west 
	corner of Lot 62:
	Date Desc.:	12/05/53	Elevation:	 18 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	116.011111	Runoff:	Rapid
	Easting/Lat.:	-31.81694444	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.5 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Channel bench	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Yellow Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.025 m	Brown (10YR5/3-Moist); ; Fine sandy loam (Fibric); Moist; Very weak consistence; 
	CommonSharp, Irregular change to - 
	A2	0.025 - 0.09 m	Yellowish brown (10YR5/4-Moist); ; Fine sandy loam; Moist; Weak consistence; FewSharp, 
	Smooth change to - 
	B1	0.09 - 0.41 m	Yellowish red (5YR4/8-Moist); ; Fine sandy medium clay; Massive grade of structure; Moist; 
	Moderately plastic; Normal plasticity; Diffuse, Smooth change to - 
	B2	0.48 - 0.96 m	Yellow (10YR7/8-Moist); , 5Y52, 2-10% ; , 2.5YR58, 2-10% ; Fine sandy medium clay; Massive 
	grade of structure; Moist; Moderately plastic; Normal plasticity; 
	D1	0.96 - 1.37 m	Grey (10YR6/1-Moist); , 10YR43; , 10YR78; Medium clay; Dry; Strong consistence; 
	D2	1.37 - 1.47 m	Brownish yellow (10YR6/8-Moist); , 10YR61; , 10YR43; Sandy medium clay; 2-10%, 
	undisturbed, Substrate material, coarse fragments; 
	Morphological Notes
	Observation Notes
	137-147CM GV FERRUGINISED:>147CM ON ROCK:                                                                               
	Site Notes
	SOUTH-WEST LD

	Project Name:	SWV
	Project Code:	SWV	Site ID:	P176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	6.5A
	0.025 - 0.09	6.2A
	0.09 - 0.41	6.5A	 2.8K	 3.5	 0.62	 0.25	 5.2E	 12.4B
	0.48 - 0.96	6.9A
	0.96 - 1.37	7.4A
	1.37 - 1.47	8.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025
	0.025 - 
	0.09
	0.09 - 0.41	 5D	 37	 10	 41
	0.48 - 0.96
	0.96 - 1.37
	1.37 - 1.47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.09
	0.09 - 0.41
	0.48 - 0.96
	0.96 - 1.37
	1.37 - 1.47

	Project Name:	SWV
	Project Code:	SWV	Site ID:	P176	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance