Project Name:	SWV
	Project Code:	SWV	Site ID:	P191	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	L.W. Pym	Locality:	Old clay pit east of junction of Northern Highway and 
	Middle Swamp RoadLoc. 13:
	Date Desc.:	11/12/53	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 2134   1:100000	Rainfall:	0
	Northing/Long.:	116.010555555556	Runoff:	Very slow
	Easting/Lat.:	-31.8641666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Pit	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Brown Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.025 m	Grey (2.5YR5/0-Moist); ; Loam (Fibric); Weak grade of structure; Dry; 2-10%, Charcoal, coarse 
	fragments; Field pH 6 (pH meter); Clear, Smooth change to - 
	A2	0.025 - 0.15 m	Brown (10YR5/3-Moist); ; Clay loam; Massive grade of structure; Dry; 2-10%, fine gravelly, 2-
	6mm, Quartz, coarse fragments; Field pH 5.5 (pH meter); Clear, Smooth change to - 
	B1	0.15 - 0.48 m	Yellowish brown (10YR5/8-Moist); , 10YR43; Medium clay; Massive grade of structure; Dry; 
	Weak consistence; 2-10%, fine gravelly, 2-6mm, rounded, Substrate material, coarse fragments;
	 Field pH 6 (pH meter); Clear, Smooth change to - 
	B1B2	0.48 - 0.66 m	Brown (10YR4/3-Moist); , 10YR58; , 10YR61; Medium clay; Massive grade of structure; Dry; 
	Weak consistence; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Few (2 - 10 
	%), Manganiferous, , Concretions; Field pH 6 (pH meter); Diffuse change to - 
	Cg	0.66 - 1.27 m	Brown (10YR4/3-Moist); , 10YR58; , 10YR61; Medium clay; Dry; Field pH 6 (pH meter); 
	C	1.27 - 1.83 m	Brown (10YR4/3-Moist); , 10YR58; , 10YR61; Medium clay; Dry; Weak consistence; 
	Morphological Notes
	Observation Notes
	15-48CM AL GV FERRUGINISED AND PISOLITIC:                                                                               
	Site Notes
	SOUTH-WEST LD

	Project Name:	SWV
	Project Code:	SWV	Site ID:	P191	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	4.8A	 0.182A	 6.29K	 1.54	 0.73	 0.64	 36.9E	 46.1B
	0.025 - 0.15	5.3A	 0.042A	 0.81K	 0.81	 0.08	 0.15	 14.7E	 16.6B
	0.15 - 0.48	5.9A	 0.036A	 3.46K	 2.54	 0.23	 0.4	 6.3E	 12.9B
	0.48 - 0.66	6.6A
	0.66 - 1.27	6.1A	 0.131A	 7.02K	 2.29	 0.15	 0.18	 4.7E	 14.3B
	1.27 - 1.83	6.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 0.023D	 0.224A	 21D	 22	 18	 13
	0.025 - 	 22D	 25	 22	 25
	0.15
	0.15 - 0.48	 19D	 20	 19	 42
	0.48 - 0.66
	0.66 - 1.27	 28D	 18	 15	 39
	1.27 - 1.83
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.15
	0.15 - 0.48
	0.48 - 0.66
	0.66 - 1.27
	1.27 - 1.83

	Project Name:	SWV
	Project Code:	SWV	Site ID:	P191	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance