Project Name:	UNI
	Project Code:	UNI	Site ID:	P358	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	Part location 2103 1(D/40):
	Date Desc.:	24/10/57	Elevation:	 23 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	115.8	Runoff:	Very rapid
	Easting/Lat.:	-31.95	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Dunefield
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Bleached Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	Ap	0 - 0.18 m	Dark grey (10YR4/1-Moist); ; Sand (Fibric); Single grain grade of structure; Diffuse change to - 
	A1	0.18 - 0.41 m	Pale red (2.5YR7/2-Moist); ; Sand; Single grain grade of structure; Diffuse change to - 
	A2	0.41 - 0.53 m	Pale yellow (2.5Y7/4-Moist); ; Sand; Diffuse change to - 
	B	0.53 - 0.94 m	Yellow (10YR7/6-Moist); , 10YR68, 2-10% ; , 2-10% ; Sand; 
	0.94 - 1.22 m	Brownish yellow (10YR6/8-Moist); ; Sand; 
	1.22 - 1.52 m	Yellow (10YR8/6-Moist); ; Sand; 
	1.52 - 1.83 m	Yellow (10YR8/8-Moist); ; Sand; 
	1.83 - 2.13 m	Yellow (10YR8/6-Moist); ; Sand; 
	2.13 - 2.44 m	Pale yellow (2.5Y8/4-Moist); ; Sand; 
	2.44 - 2.74 m	Pale yellow (2.5Y8/4-Moist); ; Sand; 
	Morphological Notes
	Observation Notes
	18-41CM ORGANIC STAINED:                                                                                                
	Site Notes
	PERTH

	Project Name:	UNI
	Project Code:	UNI	Site ID:	P358	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.18	6.7A	 0.027A
	0.18 - 0.41	6.7A	 0.012A
	0.41 - 0.53	6.8A	 0.012A
	0.53 - 0.94	6.8A	 0.018A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.18
	0.18 - 0.41
	0.41 - 0.53
	0.53 - 0.94
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.18
	0.18 - 0.41
	0.41 - 0.53
	0.53 - 0.94

	Project Name:	UNI
	Project Code:	UNI	Site ID:	P358	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour