Project Name:	WIM
	Project Code:	WIM	Site ID:	P394	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.H. Litchfield	Locality:	Near north part of location M517 Melbourne:
	Date Desc.:	26/09/58	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	Runoff:	Moderately rapid
	Easting/Lat.:	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial fan
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Duric Red Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:	Low Strata - Forb, , Closed or dense. *Species includes - None recorded
	Tall Strata - Shrub, , Closed or dense. *Species includes - Acacia aneura
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.04 m	Dark reddish brown (2.5YR3/4-Moist); Reddish brown (2.5YR4/4-Dry); ; Fine sandy medium clay 
	(Light); Strong consistence; 
	0.04 - 0.15 m	Red (2.5YR5/6-Dry); ; Fine sandy medium clay; Massive grade of structure; Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Strong consistence; 2-10%, medium gravelly, 6-20mm, 
	Substrate material, coarse fragments; Common, fine (1-2mm) roots; 
	0.15 - 0.28 m	Red (2.5YR5/6-Dry); ; Medium clay; Strong consistence; 2-10%, medium gravelly, 6-20mm, 
	Substrate material, coarse fragments; Common, fine (1-2mm) roots; 
	0.28 - 0.58 m	Red (2.5YR5/8-Dry); ; Medium clay; Strong consistence; 2-10%, medium gravelly, 6-20mm, 
	Substrate material, coarse fragments; Common, fine (1-2mm) roots; 
	0.58 - 0.84 m	Red (2.5YR5/8-Dry); ; Medium clay; Strong consistence; Common, fine (1-2mm) roots; Gradual 
	change to - 
	0.84 - 1.22 m	Red (2.5YR5/8-Dry); ; Medium clay; Strong consistence; Few (2 - 10 %), Ferruginous, Coarse (6 -
	 20 mm), Nodules; Common, fine (1-2mm) roots; 
	1.22 - 1.52 m	Light yellowish brown (10YR6/4-Moist); Reddish yellow (7.5YR6/8-Dry); , 5YR44; Medium clay; 2-
	10%, Substrate material, coarse fragments; 
	1.52 - 1.63 m	Light yellowish brown (10YR6/4-Moist); , 5Y43; , 5Y62; Medium clay; 20-50%, Substrate 
	material, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-163CM AL GV IS FERRUGINOUS: >163CM ON HARDPAN:                                                                        
	Site Notes
	WILUNA

	Project Name:	WIM
	Project Code:	WIM	Site ID:	P394	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	5.4A	 0.045A
	0.04 - 0.15	4.8A	 0.024A	 0.6K	 0.2	 0.28	 0.04
	0.15 - 0.28	4.8A	 0.018A
	0.28 - 0.58	4.7A	 0.021A
	0.58 - 0.84	4.8A	 0.018A
	0.84 - 1.22	5A	 0.015A	 0.2K	 0.7	 0.18	 0.06
	1.22 - 1.52	5A	 0.018A
	1.52 - 1.63	4.9A	 0.021A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 1.39D	 0.026D	 0.099B	 28D	 42	 6	 23
	0.04 - 0.15	 0.68D	 0.024D	 0.053B	 28D	 40	 6	 26
	0.15 - 0.28	 27D	 38	 4	 30
	0.28 - 0.58	 20D	 40	 7	 31
	0.58 - 0.84	 0.032B
	0.84 - 1.22	 0.021D	 18D	 38	 9	 34
	1.22 - 1.52	 18D	 39	 9	 31
	1.52 - 1.63
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.15
	0.15 - 0.28
	0.28 - 0.58
	0.58 - 0.84
	0.84 - 1.22
	1.22 - 1.52
	1.52 - 1.63

	Project Name:	WIM
	Project Code:	WIM	Site ID:	P394	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance