Project Name:	WOK
	Project Code:	WOK	Site ID:	P56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	L.W. Pym	Locality:	80 chains along Mornington Road:cutting in 
	Date Desc.:	21/12/50	Elevation:	 61 metres
	Map Ref.:	Sheet No. : 2031   1:100000	Rainfall:	0
	Northing/Long.:	115.8925	Runoff:	Rapid
	Easting/Lat.:	-33.1377777777778	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Peneplain
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Cutface	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Brown podzolic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.025 m	Greyish brown (10YR5/2-Moist); ; Sandy loam (Fibric); Single grain grade of structure; Diffuse, 
	Irregular change to - 
	A2	0.025 - 0.1 m	Greyish brown (10YR5/2-Moist); ; Sandy loam; Single grain grade of structure; 2-10%, Quartz, 
	coarse fragments; Diffuse, Irregular change to - 
	B2	0.1 - 0.51 m	Yellowish brown (10YR5/6-Moist); ; Medium clay; Massive grade of structure; 2-10%, Gravel, 
	coarse fragments; Diffuse, Irregular change to - 
	Morphological Notes
	Observation Notes
	10-51CM QZ + GNEISS + FERRUGINISED GV:>51CM GRITTY CLAY (W'D SCHISTOSE ROCK):                                           
	Site Notes
	HARVEY RD BD

	Project Name:	WOK
	Project Code:	WOK	Site ID:	P56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	6.2A	 0.092A	 6.3K	 3	 0.58	 10B
	6.2A	 0.13
	0.025 - 0.1	6.1A	 0.036A	 4.1K	 2.2	 0.36	 6.7B
	6.1A	 0.08
	0.1 - 0.51	6.3A	 0.03A	 3.1K	 5.3	 0.43	 8.9B
	6.3A	 0.09
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 3.98D	 0.016D	 0.24B	 3	 21D	 58	 10	 11
	0.025 - 0.1	 2.24D	 0.008D	 0.115B	 6	 15D	 59	 7	 18
	0.1 - 0.51	 1.04D	 0.009D	 0.092B	 6	 14D	 34	 7	 44
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.1
	0.1 - 0.51

	Project Name:	WOK
	Project Code:	WOK	Site ID:	P56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance