Project Name:	YRK
	Project Code:	YRK	Site ID:	P245	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	M.J. Mulcahy	Locality:	L.D. Sheet 3/80 - Block 10431:64 chains north east 
	along track from main road.
	Date Desc.:	15/08/55	Elevation:	 305 metres
	Map Ref.:	Sheet No. : 2334   1:100000	Rainfall:	430
	Northing/Long.:	117.059722222222	Runoff:	Rapid
	Easting/Lat.:	-31.9561111111111	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Igneous rock (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial fan
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Pediment	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Mesotrophic Red Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.06 m	Brown (7.5YR4/2-Moist); ; Coarse sand; Loose consistence; Sharp change to - 
	0.06 - 0.18 m	Reddish brown (2.5YR4/4-Moist); , 2.5YR46; , 5YR46; Clay loam; Massive grade of structure; 2-
	10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Diffuse change to - 
	0.18 - 0.41 m	Red (2.5YR4/6-Moist); , 5YR46; Medium clay; , Prismatic; Weak consistence; Diffuse change to
	 - 
	0.41 - 0.56 m	Yellowish red (5YR4/6-Moist); , 5YR66; , 2.5YR46; Medium clay; , Prismatic; Diffuse change to - 
	0.56 - 0.79 m	Yellowish red (5YR4/6-Moist); , 5YR66; , 10YR63; Medium clay; Massive grade of structure; Very
	 weak consistence; 2-10%, Substrate material, coarse fragments; 
	0.84 - 1.07 m	Yellowish red (5YR4/6-Moist); , 10YR63; , 5YR66; Medium clay; 
	1.07 - 1.34 m	Reddish yellow (5YR6/6-Moist); , 2.5YR48; , 7.5YR78; Loam; 
	1.5 - 1.65 m	Yellow (10YR7/6-Moist); , 10YR73; Sandy loam; 
	1.65 - 1.8 m	Very pale brown (10YR7/3-Moist); , 10YR78; , 10YR56; Sandy clay loam; 
	Morphological Notes
	Observation Notes
	Site Notes
	KAURING

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P245	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.6A	 0.071A	 3.1K	 1.7	 0.2	 0.59	 6E	 11.6B
	0.06 - 0.18	6.4A	 0.071A	 2.1K	 1.9	 0.12	 0.44	 4.1E	 8.7B
	0.18 - 0.41	6A	 0.098A
	0.41 - 0.56	4.9A	 0.098A	 0.6K	 1.9	 0.12	 0.4
	0.56 - 0.79	4.9A	 0.098A	 0.5K	 2.4	 0.14	 0.51	 5.1E	 8.7B
	0.84 - 1.07	5.1A	 0.074A
	1.07 - 1.34	5.3A	 0.054A
	1.5 - 1.65	5.5A	 0.054A
	1.65 - 1.95
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 2.41D	 0.013D	 0.09B	 11	 59D	 21	 4	 12
	0.06 - 0.18	 1.21D	 0.006D	 0.044B	 7	 52D	 17	 5	 24
	0.18 - 0.41
	0.41 - 0.56	 23	 28D	 17	 4	 50
	0.56 - 0.79	 0.003D	 10
	0.84 - 1.07	 32	 22D	 31	 10	 37
	1.07 - 1.34	 12	 28D	 42	 12	 19
	1.5 - 1.65
	1.65 - 1.95
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.18
	0.18 - 0.41
	0.41 - 0.56
	0.56 - 0.79
	0.84 - 1.07
	1.07 - 1.34
	1.5 - 1.65
	1.65 - 1.95

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P245	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance