Project Name:	YRK
	Project Code:	YRK	Site ID:	P252	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	M.J. Mulcahy	Locality:	L.D. Sheet 3/80 - Block 8613:at side of track 24 
	chains south east fromwest corner:
	Date Desc.:	17/08/55	Elevation:	No Data
	Map Ref.:	Sheet No. : 2334   1:100000	Rainfall:	0
	Northing/Long.:	117.05	Runoff:	Rapid
	Easting/Lat.:	-31.94	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Igneous rock (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red-brown earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.15 m	Dark reddish brown (2.5YR3/4-Moist); ; Coarse sandy loam; , Columnar; Weak consistence; 20-
	50%, Igneous rock (unidentified), coarse fragments; Diffuse change to - 
	0.15 - 0.33 m	Dark red (2.5YR3/6-Moist); ; Medium clay; , Granular; 20-50%, Igneous rock (unidentified), coarse
	 fragments; Diffuse change to - 
	0.33 - 0.61 m	Dark red (2.5YR3/6-Moist); ; Medium clay; , Granular; Weak consistence; 
	0.76 - 0.86 m	Yellowish red (5YR4/6-Moist); ; Medium clay; 10-20%, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	76-86CM FELSPAR FRAGMENTS ALSO:61-76CM ROCK SAMPLE AND CLAY FOR X-RAY WEATHERING SEQUENCE:           
	                   
	Site Notes
	KAURING

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P252	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6.4A	 0.065A	 5.5K	 1	 0.86	 0.28	 3.6E	 11.2B
	0.15 - 0.33	6.6A	 0.098A	 6.9K	 2.4	 0.86	 0.4	 3.3E	 13.8B
	0.33 - 0.61	6.7A	 0.226A	 10.5K	 5.1	 0.6	 0.72	 5.3E	 22.2B
	0.76 - 0.86	6.8A	 0.188A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 1.27D	 0.013D	 0.083B	 53	 41D	 9	 12
	0.15 - 0.33
	0.33 - 0.61	 0.009D	 53	 25D	 6	 42
	0.76 - 0.86	 29	 30D	 12	 24
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.33
	0.33 - 0.61
	0.76 - 0.86

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P252	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance