Project Name:	YRK
	Project Code:	YRK	Site ID:	P306	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	M.J. Mulcahy	Locality:	4.85KM from York on York-Northam Road:
	Date Desc.:	20/09/56	Elevation:	 183 metres
	Map Ref.:	Sheet No. : 2234   1:100000	Rainfall:	460
	Northing/Long.:	116.791944444445	Runoff:	Rapid
	Easting/Lat.:	-31.8622222222222	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Diorite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Lithocalcic Brown Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Brown clay
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.15 m	Dark brown (7.5YR3/2-Moist); ; Clay loam; , Columnar; Strong consistence; 2-10%, medium 
	gravelly, 6-20mm, Quartz, coarse fragments; Few (2 - 10 %), Calcareous, , Concretions; Sharp 
	change to - 
	0.15 - 0.3 m	Reddish brown (5YR4/3-Moist); ; Medium clay; , Columnar; Weak consistence; 2-10%, Quartz, 
	coarse fragments; 
	0.41 - 0.76 m	Brown (7.5YR4/4-Moist); , 10YR82; Medium clay; ; FragmentWeak consistence; 2-10%, Quartz, 
	coarse fragments; Many (20 - 50 %), Calcareous, , Concretions; 
	0.76 - 1.09 m	Light brown (7.5YR6/4-Moist); , 10YR82; Medium clay; 2-10%, Quartz, coarse fragments; Very 
	many (50 - 100 %), Calcareous, , Concretions; 
	1.09 - 1.52 m	Light brown (7.5YR6/4-Moist); , 10YR82; Medium clay; 2-10%, Quartz, coarse fragments; Many 
	(20 - 50 %), Calcareous, , Concretions; 
	1.98 - 2.08 m	Light brown (7.5YR6/4-Moist); ; Medium clay; Few (2 - 10 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	15-76CM <10% EPIDIORITE STONES ALSO:                                                                                    
	Site Notes
	YORK

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P306	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	8.1A	 0.125A
	0.15 - 0.3	8.5A	 0.11A
	0.41 - 0.76	9.5A	 0.232A
	0.76 - 1.09	9.9A	 0.042A
	1.09 - 1.52	8.6A	 0.667A
	1.98 - 2.08	8.4A	 1.34A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 2.59A	 1.45D	 0.016D	 0.122B	 23	 32D	 28	 5	 27
	0.15 - 0.3	 0.13A	 0.007D	 35	 35D	 22	 3	 34
	0.41 - 0.76	 11.5A	 27	 30D	 22	 4	 31
	0.76 - 1.09	 21A	 0.005D	 13	 26D	 19	 3	 26
	1.09 - 1.52	 16A	 29	 27D	 21	 4	 28
	1.98 - 2.08	 3A	 0.003D	 5	 27D	 26	 6	 35
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.41 - 0.76
	0.76 - 1.09
	1.09 - 1.52
	1.98 - 2.08

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P306	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance