Project Name:	BUR
	Project Code:	BUR	Site ID:	H97	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J. Loveday	Locality:	1.6km SW of Lapoinya:
	Date Desc.:	23/03/54	Elevation:	 366 metres
	Map Ref.:	Sheet No. : 8015   1:100000	Rainfall:	1220
	Northing/Long.:	145.55	Runoff:	Rapid
	Easting/Lat.:	-41.0166666666667	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	14.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Humose-Acidic Dystrophic Red Ferrosol     	Principal Profile Form:	Gn4.11
	ASC Confidence:	Great Soil Group:	Krasnozem
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Yellowish red (5YR3/6-Moist); ; Clay loam; Strong grade of structure, Granular; Weak 
	consistence; 0-2%, stony, 200-600mm, Basalt, coarse fragments; Abundant, fine (1-2mm) roots;
	 Diffuse change to - 
	0.08 - 0.15 m	Brown (7.5YR4/4-Moist); ; Clay loam; Strong grade of structure, Granular; Weak consistence; 0-
	2%, stony, 200-600mm, Basalt, coarse fragments; Sharp change to - 
	0.15 - 0.28 m	Dark reddish brown (5YR3/4-Moist); ; Heavy clay; Strong grade of structure, Granular; Weak 
	consistence; 0-2%, stony, 200-600mm, Basalt, coarse fragments; Diffuse change to - 
	0.28 - 0.41 m	Yellowish red (5YR3/6-Moist); ; Heavy clay; Strong grade of structure, Granular; Weak 
	consistence; 0-2%, stony, 200-600mm, Basalt, coarse fragments; Few (2 - 10 %), Argillaceous, 
	, Nodules; Diffuse change to - 
	0.41 - 0.56 m	Yellowish red (5YR3/6-Moist); ; Heavy clay; Moderate grade of structure, Granular; Weak 
	consistence; 2-10%, coarse gravelly, 20-60mm, Basalt, coarse fragments; Very few (0 - 2 %), 
	Unidentified, Fine (0 - 2 mm), Concretions; Diffuse change to - 
	0.56 - 0.71 m	Dark red (2.5YR3/6-Moist); ; Heavy clay; Massive grade of structure; Firm consistence; Few (2 - 
	10 %), Manganiferous, Fine (0 - 2 mm), Concretions; Diffuse change to - 
	0.76 - 0.91 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Massive grade of structure; Very weak consistence; 
	Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Concretions; Diffuse change to - 
	0.99 - 1.17 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Massive grade of structure; Very weak consistence; 
	2-10%, medium gravelly, 6-20mm, Basalt, coarse fragments; Few (2 - 10 %), Unidentified, 
	Medium (2 -6 mm), Concretions; Diffuse change to - 
	1.68 - 1.78 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Massive grade of structure; Weak consistence; 2-
	10%, Basalt, coarse fragments; 
	2.54 - 2.74 m	; 
	Morphological Notes
	Purple (5R2/6) mealy decomposed ba with YB and BL staining:
	Observation Notes
	8-15CM MANY WORMS:168-178CM YELLOW-WHITE MATERIAL ALSO:>274CM DECOMPOSING BA MORE 

	Project Name:	BUR
	Project Code:	BUR	Site ID:	H97	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Notes
	WELLINGTON

	Project Name:	BUR
	Project Code:	BUR	Site ID:	H97	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.8A	 28C
	0.08 - 0.15	5.2A	 3.5H	 1.9	 0.15	 0.21	 21.7H	 49.2B
	 43.4E
	0.15 - 0.28	5.1A	 19.5C
	0.28 - 0.41	5.2A	 1.9H	 0.78	 0.12	 0.14	 16.6H	 35.9B
	 33E
	0.41 - 0.56	5A	 16.5C
	0.56 - 0.71	5.1A	 1.2H	 0.65	 0.09	 0.08	 14.9H	 30.8B
	 28.8E
	0.76 - 0.91	4.8A
	0.99 - 1.17	4.7A	 13C
	1.68 - 1.78	4.8A
	2.54 - 2.74	4.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 6.1D	 0.148D	 0.556A
	0.08 - 0.15	 4.9D	 0.129D	 0.426A	 1	 4B	 23	 25	 36
	0.15 - 0.28	 3.5D	 0.096D	 0.322A
	0.28 - 0.41	 2.7D	 0.069D	 0.264A	 0	 2B	 8	 17	 72
	0.41 - 0.56	 2.1D	 0.19A
	0.56 - 0.71	 1.2D	 0.072D	 0	 2B	 8	 15	 74
	0.76 - 0.91
	0.99 - 1.17	 0.3D
	1.68 - 1.78
	2.54 - 2.74
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.28
	0.28 - 0.41
	0.41 - 0.56
	0.56 - 0.71
	0.76 - 0.91
	0.99 - 1.17
	1.68 - 1.78
	2.54 - 2.74

	Project Name:	BUR
	Project Code:	BUR	Site ID:	H97	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette