Project Name:	DER
	Project Code:	DER	Site ID:	H205	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	On western side of Richmond H`way:4.85KM SSW of 
	Richmond on property "Lauderdale":4.6M from fence 
	line:
	Date Desc.:	14/12/60	Elevation:	 21 metres
	Map Ref.:	Rainfall:	580
	Northing/Long.:	147.411111111111	Runoff:	Moderately rapid
	Easting/Lat.:	-42.7763888888889	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.4 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Vertic Eutrophic Brown Kurosol     	Principal Profile Form:	Db2.41
	ASC Confidence:	Great Soil Group:	Soloth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); Grey (10YR5/1-Dry); ; Loamy sand; Massive grade of structure; 
	Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Strong consistence; 2-10%, coarse 
	gravelly, 20-60mm, rounded, Mudstone, coarse fragments; CommonDiffuse change to - 
	A1	0.1 - 0.18 m	Very dark grey (10YR3/1-Moist); Grey (10YR5/1-Dry); ; Loamy sand; Massive grade of structure; 
	Few (<1 per 100mm2) Fine (1-2mm) macropores, Dry; Strong consistence; 2-10%, coarse 
	gravelly, 20-60mm, rounded, Mudstone, coarse fragments; CommonSharp change to - 
	A2sb	0.19 - 0.28 m	Dark grey (10YR4/1-Moist); Light grey (10YR7/1-Dry); ; Loamy sand; Massive grade of structure; 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Strong consistence; 2-10%, coarse 
	gravelly, 20-60mm, rounded, Mudstone, coarse fragments; 
	B	0.33 - 0.43 m	Dark greyish brown (2.5Y4/3-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Strong consistence; 2-10%, coarse gravelly, 20-60mm, 
	rounded, Mudstone, coarse fragments; 
	B	0.2 - 0.36 m	Very dark grey (10YR3/1-Moist); , 2.5Y43; , 10YR44; Heavy clay; Strong grade of structure, 20-50 
	mm, Angular blocky; Dry; Very strong consistence; 2-10%, coarse gravelly, 20-60mm, rounded, 
	Mudstone, coarse fragments; Diffuse change to - 
	B	0.36 - 0.43 m	Dark greyish brown (2.5Y4/3-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moderately moist; Strong consistence; 2-10%, coarse gravelly, 20-60mm, 
	rounded, Mudstone, coarse fragments; Sharp change to - 
	0.46 - 0.63 m	Dark greyish brown (2.5Y4/3-Moist); , 10YR44; , 10YR31; Heavy clay; Weak grade of structure, 
	20-50 mm, Angular blocky; Firm consistence; Slightly plastic; Normal plasticity; 2-10%, coarse 
	gravelly, 20-60mm, rounded, Mudstone, coarse fragments; Sharp change to - 
	0.66 - 0.89 m	Olive (5Y5/3-Moist); , 5Y63; , 7.5YR58; Heavy clay; Massive grade of structure; Weak 
	consistence; Slightly plastic; Normal plasticity; 20-50%, coarse gravelly, 20-60mm, rounded, 
	Mudstone, coarse fragments; Sharp change to - 
	0.91 - 1.09 m	Olive grey (5Y5/2-Moist); , 10YR58; Sandy medium clay; Massive grade of structure; Weak 
	consistence; 

	Project Name:	DER
	Project Code:	DER	Site ID:	H205	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	1.32 - 1.42 m	Olive (5Y5/3-Moist); ; Sandy medium clay; Weak consistence; 50-90%, cobbly, 60-200mm, 
	rounded, Dolerite, coarse fragments; 
	Morphological Notes
	Observation Notes
	33-43CM 10YR31 COATING ON AGGREGATES:0-28CM <10% CHARCOAL ALSO:BLEACHEDA2 DEVELOPED IN CLAY 
	DEPRESSIONS "ISLANDS":      
	Site Notes
	HOBART

	Project Name:	DER
	Project Code:	DER	Site ID:	H205	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9A	 0.045A	 4H	 0.99	 0.15	 6.6H	 15B
	 9.6E
	0.1 - 0.18	5.3A	 0.027A	 3.3H	 0.94	 0.18	 6.3H	 12.8B
	 8.3E
	0.19 - 0.28	5.8A	 0.024A	 1.3H	 0.81	 1.5	 3.3H	 7.3B
	 4.9E
	0.33 - 0.43	5.2A	 0.086A	 1.8H	 7.4	 1	 15H	 29.7B
	 18.5E
	0.2 - 0.36	5.2A	 0.06A	 3.9H	 7.1	 14.4H	 31.5B
	 19.1E
	0.36 - 0.43	5.1A	 0.086A	 1.9
	0.46 - 0.63	5.2A	 0.107A	 1.9H	 8.6	 12.4H	 28.3B
	 15.4E
	0.66 - 0.89	5.2A	 0.134A
	0.91 - 1.09	5.4A	 0.131A
	1.32 - 1.42	5.8A	 0.196A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.66D	 0.016D	 0.151A	 18	 27B	 50	 10	 8
	0.1 - 0.18	 2.07D	 0.011D	 0.105A	 2	 30D	 48	 11	 8
	0.19 - 0.28	 0.62D	 0.028A	 1	 27D	 48	 12	 11
	0.33 - 0.43	 0.6D	 0.004D	 0.044A	 1	 13D	 32	 6	 46
	0.2 - 0.36	 0.72D	 0.056A	 4	 14D	 30	 7	 47
	0.36 - 0.43
	0.46 - 0.63	<1	 17D	 38	 6	 39
	0.66 - 0.89
	0.91 - 1.09
	1.32 - 1.42
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.18
	0.19 - 0.28
	0.33 - 0.43
	0.2 - 0.36
	0.36 - 0.43
	0.46 - 0.63
	0.66 - 0.89
	0.91 - 1.09
	1.32 - 1.42

	Project Name:	DER
	Project Code:	DER	Site ID:	H205	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette