Project Name:	FLI
	Project Code:	FLI	Site ID:	H46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	1.2km ENE from Thule:4.1km from Whitemark
	Date Desc.:	10/12/52	Elevation:	 91 metres
	Map Ref.:	Sheet No. : 8517   1:100000	Rainfall:	820
	Northing/Long.:	148.066666666667	Runoff:	Very slow
	Easting/Lat.:	-40.1166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic-Mottled Self-Mulching Aquic Vertosol     	Principal Profile Form:	Ug5.16
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	2-10%, bouldery, 600mm-2m, , Basalt
	Profile Morphology
	A	0 - 0.05 m	Very dark grey (10YR3/1-Moist); ; Loam; Moderate grade of structure, Granular; Moderately moist; 
	Weak consistence; 0-2%, Charcoal, coarse fragments; Very few (0 - 2 %), Unidentified, Fine (0 - 
	2 mm), Concretions; Abundant, fine (1-2mm) roots; Diffuse change to - 
	A	0.05 - 0.13 m	Very dark grey (10YR3/1-Moist); ; Light clay; Weak grade of structure, Granular; Moderately moist;
	 Weak consistence; 2-10%, medium gravelly, 6-20mm, Basalt, coarse fragments; Few (2 - 10 
	%), Unidentified, , Concretions; CommonDiffuse change to - 
	AB	0.13 - 0.2 m	Very dark grey (10YR3/1-Moist); , 10YR56, 2-10% ; , 2-10% ; Heavy clay; Weak grade of structure,
	 2-5 mm, Granular; Moist; Weak consistence; 2-10%, medium gravelly, 6-20mm, Basalt, coarse 
	fragments; Few (2 - 10 %), Unidentified, , Concretions; Diffuse change to - 
	B	0.2 - 0.33 m	Dark grey (10YR4/1-Moist); , 10YR56; , 5Y52; Heavy clay; Massive grade of structure; Moist; Very
	 weak consistence; 2-10%, cobbly, 60-200mm, Basalt, coarse fragments; Few (2 - 10 %), 
	Unidentified, , Concretions; Diffuse change to - 
	B	0.41 - 0.56 m	Dark grey (10YR4/1-Moist); , 10YR56; , 5Y52; Heavy clay; Massive grade of structure; Moist; Very
	 weak consistence; 2-10%, cobbly, 60-200mm, Basalt, coarse fragments; Few (2 - 10 %), 
	Unidentified, , Concretions; Diffuse change to - 
	B	0.56 - 0.69 m	Dark grey (10YR4/1-Moist); , 10YR56; , 5Y52; Heavy clay; Massive grade of structure; Moist; Very
	 weak consistence; 2-10%, medium gravelly, 6-20mm, Basalt, coarse fragments; Few (2 - 10 %),
	 Unidentified, , Concretions; Diffuse change to - 
	0.74 - 0.86 m	Yellowish brown (10YR5/4-Moist); , 10YR71; Heavy clay; Massive grade of structure; Slightly 
	plastic; Normal plasticity; 2-10%, Basalt, coarse fragments; Very few (0 - 2 %), Ferruginous, 
	Medium (2 -6 mm), Nodules; Diffuse change to - 
	0.99 - 1.19 m	Light brownish grey (2.5Y6/2-Moist); , 10YR66; Heavy clay; Massive grade of structure; Slightly 
	plastic; Normal plasticity; 0-2%, coarse fragments; Diffuse change to - 
	1.63 - 1.78 m	Yellowish brown (10YR5/4-Moist); , 10YR56; , 10YR71; Heavy clay; Massive grade of structure; 
	Weak consistence; 
	Morphological Notes
	Observation Notes
	13-20CM <2% CHARCOAL ALSO:                                                                                              

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	METTA
	Site Notes

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6A	 37H	 17.3	 4.4	 2.4	 29.3H	 112.2B
	 51.1E
	0.05 - 0.13	6.4A	 30.6H	 14.8	 4.7	 2.2	 15.2H	 81.3B
	 29E
	0.13 - 0.2	6.7A	 24.3H	 16.3	 2.8	 1.4	 8.4H	 66.9B
	 22.1E
	0.2 - 0.33	6.8A
	0.41 - 0.56	7A	 42.5C
	0.56 - 0.69	7.7A	 10.5H	 10.3	 1.69	 3	 6.8E	 32.3B
	0.74 - 0.86	7A
	0.99 - 1.19	5.8A
	1.63 - 1.78	5.1A	 7.4H	 21.6	 1.5	 13.7	 14.1H	 69.8B
	 25.6E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 11.3D	 0.068D	 1.07A	 3	 10B	 7	 17	 48
	0.05 - 0.13	 5.05D	 0.47A	 10	 13B	 12	 14	 53
	0.13 - 0.2	 3.32D	 0.339A	 4	 15B	 10	 10	 58
	0.2 - 0.33	 2D	 0.19A
	0.41 - 0.56	 1.3D
	0.56 - 0.69	 0.04A	 1.2D	 14	 25B	 15	 9	 47
	0.74 - 0.86
	0.99 - 1.19
	1.63 - 1.78	 0	 1B	 13	 34	 49
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.13
	0.13 - 0.2
	0.2 - 0.33
	0.41 - 0.56
	0.56 - 0.69
	0.74 - 0.86
	0.99 - 1.19
	1.63 - 1.78

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H46	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette