Project Name:	FLI
	Project Code:	FLI	Site ID:	H56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	Near site 53 on Bootjack survey:5.3km NW of Lady 
	Barron.
	Date Desc.:	15/04/53	Elevation:	 16 metres
	Map Ref.:	Sheet No. : 8517   1:100000	Rainfall:	750
	Northing/Long.:	148.2	Runoff:	No runoff
	Easting/Lat.:	-40.1833333333333	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Lagoon	Slope Category:	Level
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Lithocalcic Grey Chromosol     	Principal Profile Form:	Dd2.33
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:	Low Strata - Sedge, 0.26-0.5m, Sparse. *Species includes - None recorded
	Tall Strata - Shrub, 1.01-3m, Isolated plants. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.04 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; Massive grade of structure; Moderately moist;
	 Weak consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 
	Abundant, fine (1-2mm) roots; Diffuse change to - 
	A1A2	0.04 - 0.08 m	Greyish brown (10YR5/2-Moist); ; Sandy loam; Massive grade of structure; Moderately moist; 
	Weak consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; 
	Abundant, fine (1-2mm) roots; Diffuse change to - 
	A2	0.08 - 0.18 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Moderately moist; Loose
	 consistence; 2-10%, fine gravelly, 2-6mm, rounded, stratified, Gravel, coarse fragments; 
	Irregular change to - 
	B	0.13 - 0.16 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; Strong grade of structure, 100-200 mm, 
	Columnar; Fine, (0 - 5) mm crack; Moderately moist; Very firm consistence; 2-10%, fine gravelly, 
	2-6mm, rounded, Quartz, coarse fragments; 
	B	0.16 - 0.23 m	Dark greyish brown (10YR4/2-Moist); , 10YR54; Heavy clay; Strong grade of structure, 100-200 
	mm, Columnar; Fine, (0 - 5) mm crack; Moderately moist; Very firm consistence; 2-10%, fine 
	gravelly, 2-6mm, rounded, Quartz, coarse fragments; CommonDiffuse change to - 
	B	0.23 - 0.32 m	Very dark greyish brown (10YR3/2-Moist); , 10YR54; Heavy clay; Strong grade of structure, 100-
	200 mm, Columnar; Fine, (0 - 5) mm crack; Moderately moist; Very firm consistence; 2-10%, fine
	 gravelly, 2-6mm, rounded, Quartz, coarse fragments; 
	B	0.34 - 0.52 m	Very dark grey (10YR3/1-Moist); , 10YR78; Heavy clay; Weak grade of structure, 100-200 mm, 
	Columnar; Fine, (0 - 5) mm crack; Moist; Very firm consistence; 2-10%, fine gravelly, 2-6mm, 
	rounded, Quartz, coarse fragments; 
	B	0.58 - 0.69 m	Dark grey (10YR4/1-Moist); , 10YR66; Heavy clay; Massive grade of structure; Fine, (0 - 5) mm 
	crack; Moist; Firm consistence; 10-20%, fine gravelly, 2-6mm, rounded, Quartz, coarse 
	fragments; 
	B	0.72 - 0.84 m	Dark grey (10YR4/1-Moist); , 10YR68; Heavy clay; Massive grade of structure; Moist; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, rounded, Quartz, coarse fragments; 

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	B	0.89 - 1.04 m	Grey (10YR5/1-Moist); , 10YR68; , 10YR81; Heavy clay; Massive grade of structure; Moist; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, rounded, Quartz, coarse fragments; Many (20 - 50 %), 
	Calcareous, Extremely coarse (> 60 mm), Concretions; 
	1.68 - 1.83 m	Dark bluish grey (5B4/1-Moist); , 5B61; , 10YR78; Heavy clay (Light); Slightly plastic; Normal 
	plasticity; 2-10%, fine gravelly, 2-6mm, Gravel, coarse fragments; 
	2.51 - 2.59 m	Greenish grey (5G6/1-Moist); ; Sandy medium clay; Very weak consistence; 0-2%, Gravel, coarse
	 fragments; 
	Morphological Notes
	Observation Notes
	193-228CM <2% <6MM ROUNDED QZ GV:0-183CM COARSE FRACTION ALL OF GRIT SIZE:BOOTJACK SERIES:                    
	          
	Site Notes
	COOMA

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	6A	 9.9H	 3.8	 0.54	 0.81	 5.3H	 25.7B
	 10.5E
	0.04 - 0.08	6.4A
	0.08 - 0.18	6.4A	 2H	 0.88	 0.08	 0.16	 1.3H	 5.4B
	 2.3E
	0.13 - 0.16	6.2A	 6.2H	 3.7	 0.2	 0.82	 1.8H	 15.2B
	 4.3E
	0.16 - 0.23	6.7A
	0.23 - 0.32	7.1A	 8.8H	 6	 0.2	 1.7	 4.2E	 20.9B
	0.34 - 0.52	7.7A
	0.58 - 0.69	7.9A	 6.1H	 4.6	 0.21	 1.5	 1.7E	 14.1B
	0.72 - 0.84	7.9A
	0.89 - 1.04	8.4A
	1.68 - 1.83	7.8A
	2.51 - 2.59	8.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 3.7D	 0.003D	 0.254A	 1	 39B	 31	 10	 14
	0.04 - 0.08	 1.92D
	0.08 - 0.18	 0.74D	 0.001D	 0.065A	 6	 62B	 26	 5	 6
	0.13 - 0.16	 1.49D	 0.001D	 0.11A	 9	 55B	 19	 4	 22
	0.16 - 0.23	 1.44D	 0.119A
	0.23 - 0.32	 1.08D	 0.097A	 5	 43B	 18	 7	 31
	0.34 - 0.52	 0.03A	 0.8D
	0.58 - 0.69	 0.02A	 32D	 0.001D	 13	 49B	 17	<1	 34
	0.72 - 0.84	 0.03A
	0.89 - 1.04	 0.61A
	1.68 - 1.83	 0.02A
	2.51 - 2.59	 0.22A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.08
	0.08 - 0.18
	0.13 - 0.16
	0.16 - 0.23
	0.23 - 0.32
	0.34 - 0.52
	0.58 - 0.69
	0.72 - 0.84
	0.89 - 1.04
	1.68 - 1.83
	2.51 - 2.59

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H56	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette