Project Name:	FLI
	Project Code:	FLI	Site ID:	H60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:	1.6km S of Killiecrankie t`off:
	Date Desc.:	19/04/53	Elevation:	 91 metres
	Map Ref.:	Sheet No. : 8418   1:100000	Rainfall:	710
	Northing/Long.:	147.866666666667	Runoff:	Rapid
	Easting/Lat.:	-39.8666666666667	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Silpanic Bleached-Leptic Tenosol     	Principal Profile Form:	Dg3.81
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Sedge, <0.25m, Sparse. *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	20-50%, fine gravelly, 2-6mm, angular, Quartz
	Profile Morphology
	A1/A2	0 - 0.04 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Moist; Very weak 
	consistence; 20-50%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; CommonDiffuse 
	change to - 
	A2	0.04 - 0.15 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Moist; Very weak 
	consistence; 50-90%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; CommonDiffuse 
	change to - 
	A2	0.15 - 0.3 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Moderately moist; 
	Loose consistence; 50-90%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; 
	FewDiffuse change to - 
	A2	0.3 - 0.51 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Moderately moist; 
	Loose consistence; 50-90%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Sharp 
	change to - 
	0.51 - 0.79 m	White (10YR8/1-Moist); ; Clayey sand; Massive grade of structure; Fine, (0 - 5) mm crack; 10-
	20%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Duripan, Strongly cemented, 
	Massive; Few
	Morphological Notes
	Observation Notes
	COARSE FRACTION IS OF A GRITTY NATURE:BOYES SERIES:                                                                     
	Site Notes
	LIAPOTA

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	4.7A	 1H	 0.6	 0.14	 0.05	 4.8H	 8.7B
	 6.9E
	0.04 - 0.15	4.6A	 4C
	0.15 - 0.3	4.6A	 0.11H
	0.3 - 0.51	4.8A	 2E
	0.51 - 0.79	4.4A	 0.3	 0.04	 0.03	 1H	 1.12B
	 1.65E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 1.94D	 0.001D	 0.064A	 32	 52B	 35	 6	 3
	0.04 - 0.15	 0.92D	 0.031A	 43	 62B	 30	 4	 3
	0.15 - 0.3	 0.38D	 0.013A
	0.3 - 0.51
	0.51 - 0.79	 0.002D	 19	 45B	 26	 17	 13
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.15
	0.15 - 0.3
	0.3 - 0.51
	0.51 - 0.79

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H60	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette