Project Name:	FLI
	Project Code:	FLI	Site ID:	H63	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:
	Date Desc.:	21/04/53	Elevation:	 146 metres
	Map Ref.:	Sheet No. : 8418   1:100000	Rainfall:	710
	Northing/Long.:	147.933333333333	Runoff:	Rapid
	Easting/Lat.:	-39.75	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Calcareous sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Dunefield
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcareous Regolithic Bleached Tenosol     	Principal Profile Form:	Uc4.22
	ASC Confidence:	Great Soil Group:	Calcareous sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Fern, 0.26-0.5m, Closed or dense. *Species includes - Pteridium esculentum
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Greyish brown (10YR5/2-Moist); ; Loamy sand; Single grain grade of structure; Moist; Very weak 
	consistence; AbundantDiffuse change to - 
	A1	0.1 - 0.23 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; Diffuse change to - 
	A2	0.23 - 0.38 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; Diffuse, Irregular change to - 
	A2BC	0.38 - 0.48 m	Dark brown (10YR3/3-Moist); ; Sand; Single grain grade of structure; Moderately moist; Loose 
	consistence; 2-10%, Shells, coarse fragments; 
	BC	0.58 - 0.89 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Moderately moist; 
	Very weak consistence; 10-20%, Shells, coarse fragments; Diffuse change to - 
	C	1.57 - 1.65 m	Very pale brown (10YR7/4-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; 
	C	2.59 - 2.69 m	Very pale brown (10YR7/4-Moist); ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; 
	Morphological Notes
	Observation Notes
	5.7KM ENE FROM PALANA ON NOSE OF HIGH DUNE WITH E-W TREND:LUGHRATA SERIES:                                              
	Site Notes
	PALAMA

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H63	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.1A
	0.1 - 0.23	7.2A
	0.23 - 0.38	7.6A
	0.38 - 0.48	7.9A
	0.58 - 0.89	8.9A
	1.57 - 1.65	8.7A
	2.59 - 2.69	9.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.17D	 0.005D	 0.15A
	0.1 - 0.23	 0.53D	 0.039A
	0.23 - 0.38	 0.21A	 0.27D
	0.38 - 0.48	 9.6A	 0.49D
	0.58 - 0.89	 20.8A
	1.57 - 1.65	 21.5A
	2.59 - 2.69	 26.5A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.23
	0.23 - 0.38
	0.38 - 0.48
	0.58 - 0.89
	1.57 - 1.65
	2.59 - 2.69

	Project Name:	FLI
	Project Code:	FLI	Site ID:	H63	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	12_HCL_CU	Total element - Cu(mg/kg) - Total acid(HCl)
	12_HCL_MN	Total element - Mn(mg/kg) - Total acid(HCl)
	12_HCL_ZN	Total element - Zn(mg/kg) - Total acid(HCl)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl