Project Name:	HEL
	Project Code:	HEL	Site ID:	H132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J. Loveday	Locality:	4.5KM west of Takone:
	Date Desc.:	17/01/56	Elevation:	 579 metres
	Map Ref.:	Sheet No. : 8015   1:100000	Rainfall:	1900
	Northing/Long.:	145.5625	Runoff:	Rapid
	Easting/Lat.:	-41.1666666666667	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plateau
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Humose-Acidic Dystrophic Red Ferrosol     	Principal Profile Form:	Gn4.11
	ASC Confidence:	Great Soil Group:	Krasnozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Fern, 0.51-1m, Mid-dense. *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	O1	0 - 0.03 m	Organic Layer; Very dark greyish brown (10YR3/2-Moist); ; Loam (Fibric); Diffuse change to - 
	A	0.03 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Subangular blocky;
	 Moderately moist; Weak consistence; 2-10%, Basalt, coarse fragments; Many, fine (1-2mm) 
	roots; Diffuse change to - 
	B	0.1 - 0.2 m	Brown (7.5YR4/4-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, Subangular blocky; 
	Moderately moist; Weak consistence; 2-10%, Basalt, coarse fragments; AbundantDiffuse 
	change to - 
	B	0.2 - 0.36 m	Dark reddish brown (5YR3/4-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, 
	Subangular blocky; Moderately moist; Weak consistence; 2-10%, Basalt, coarse fragments; 
	Diffuse change to - 
	BC	0.43 - 0.53 m	Brown (7.5YR4/4-Moist); ; Medium clay; Strong grade of structure, 2-5 mm, Subangular blocky; 
	Moderately moist; Weak consistence; 2-10%, Basalt, coarse fragments; , Manganiferous, Fine 
	(0 - 2 mm), Concretions; Diffuse change to - 
	C	0.56 - 0.64 m	Dark yellowish brown (10YR4/4-Moist); ; Medium clay; Weak grade of structure, Granular; Moist; 
	Weak consistence; Slightly plastic; Normal plasticity; 2-10%, Basalt, coarse fragments; , 
	Manganiferous, Fine (0 - 2 mm), Concretions; Diffuse change to - 
	C	0.71 - 0.86 m	Very dark greyish brown (10YR3/2-Moist); ; Medium clay; Weak grade of structure, Granular; 
	Moist; Weak consistence; Slightly plastic; Normal plasticity; 2-10%, Basalt, coarse fragments; ,
	 Manganiferous, Fine (0 - 2 mm), Concretions; Diffuse change to - 
	C	0.96 - 1.19 m	Dark yellowish brown (10YR3/4-Moist); ; Medium clay; Weak grade of structure, Granular; Moist; 
	Weak consistence; Slightly plastic; Normal plasticity; , Manganiferous, , Concretions; Diffuse 
	change to - 
	C	1.32 - 1.52 m	Dark yellowish brown (10YR3/4-Moist); ; Medium clay; Weak grade of structure, Granular; Weak 
	consistence; , Manganiferous, , Concretions; Diffuse change to - 
	Morphological Notes
	Observation Notes
	96-152CM WHITE GRANULES OF HALLOYSITE:                                                                                  
	Site Notes

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	BURNIE

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	4.9A
	0.03 - 0.1	5A	 2.4H	 2.4	 0.4	 0.29	 32.8H	 68B
	 62.5E
	0.1 - 0.2	4.9A	 1.1H	 1.5	 0.19	 0.15	 28.8H	 54.7B
	 51.8E
	0.2 - 0.36	4.6A
	0.43 - 0.53	4.7A	 0.1H	 0.28	 0.2	 0.17	 21.6H	 44.6B
	 43.8E
	0.56 - 0.64	4.4A
	0.71 - 0.86	4.2A
	0.96 - 1.19	4.5A
	1.32 - 1.52	4.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 28D	 0.103D	 1.52A
	0.03 - 0.1	 9.4D	 0.1D	 0.558A	 1B	 6	 14	 57
	0.1 - 0.2	 6.1D	 0.095D	 0.24A	 2B	 6	 11	 64
	0.2 - 0.36	 3.5D
	0.43 - 0.53	 1.7D	 0.102D	 0.105A	 3B	 15	 19	 54
	0.56 - 0.64
	0.71 - 0.86
	0.96 - 1.19
	1.32 - 1.52
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.1
	0.1 - 0.2
	0.2 - 0.36
	0.43 - 0.53
	0.56 - 0.64
	0.71 - 0.86
	0.96 - 1.19
	1.32 - 1.52

	Project Name:	HEL
	Project Code:	HEL	Site ID:	H132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette