Project Name:	HOB
	Project Code:	HOB	Site ID:	H22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	J.K. Taylor	Locality:	10m from Longview Avenue within lot 15:Sandy Bay:
	Date Desc.:	18/01/52	Elevation:	 91 metres
	Map Ref.:	Sheet No. : 8312   1:100000	Rainfall:	650
	Northing/Long.:	147.35	Runoff:	Rapid
	Easting/Lat.:	-42.9166666666667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 1.1 m deep,Dolerite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	17 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Epipedal Black Vertosol     	Principal Profile Form:	Ug5.13
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	Highly disturbed, for example, quarrying, roadworks, mining, landfill, urban
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.13 m	Black (10YR2/1-Moist); ; Light clay; 5-10 mm, Granular; <2 mm, Granular; Firm consistence; 0-
	2%, medium gravelly, 6-20mm, Dolerite, coarse fragments; Diffuse change to - 
	0.13 - 0.25 m	Black (10YR2/1-Moist); ; Heavy clay; 20-50 mm, Angular blocky; Moderately plastic; Normal 
	plasticity; 0-2%, Gravel, coarse fragments; Diffuse change to - 
	0.28 - 0.48 m	Very dark greyish brown (2.5Y3/2-Moist); , 5Y81; Heavy clay; , Columnar; Moderately plastic; 
	Normal plasticity; 2-10%, medium gravelly, 6-20mm, Dolerite, coarse fragments; Diffuse change
	 to - 
	0.51 - 0.61 m	Dark greyish brown (2.5Y4/2-Moist); , 5Y81; Heavy clay; Weak consistence; 0-2%, Dolerite, 
	coarse fragments; Few (2 - 10 %), Calcareous, , ; Diffuse change to - 
	0.61 - 0.89 m	Yellow (2.5Y7/6-Moist); ; Heavy clay; Very weak consistence; Common (10 - 20 %), Calcareous, 
	, Concretions; Diffuse change to - 
	0.89 - 1.09 m	; 
	Morphological Notes
	Mealy LYG decomposed dolerite
	Observation Notes
	89-109CM MEALY DECOMPOSED DOLERITE:                                                                                     
	Site Notes
	BUCKINGHAM

	Project Name:	HOB
	Project Code:	HOB	Site ID:	H22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6.8A	 28.5H	 17.2	 0.32	 0.94	 6.3H	 58.7B
	 11.7E
	0.13 - 0.25	7.2A	 33.1H	 18.4	 0.16	 1.37	 7.4E	 60.4B
	0.28 - 0.48	7.7A	 27H	 22.7	 0.09	 1.8	 3.9E	 55.5B
	0.51 - 0.61	8.4A
	0.61 - 0.89	8.8A	 32.2H	 28.2	 0.09	 3.9	 64.4B
	0.89 - 1.09	8.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 6.8F	 0.01D	 0.381A	 1	 7D	 34	 15	 40
	 4.3D
	0.13 - 0.25	 0C	 3.3F	 0.007D	 0.202A	 2	 5B	 29	 11	 50
	 2D
	0.28 - 0.48	 0.002A	 1.26F	 0.005D	 0.095A	 0	 9D	 25	 11	 57
	 0.9D
	0.51 - 0.61	 0.01A	 0.52F	 0.035A	 1	 11B	 22	 13	 49
	 0.4D
	0.61 - 0.89	 0.23A	 0.2D	 0.022A	 0	 23B	 22	 23	 30
	0.89 - 1.09	 3.22A	 0.2D	 18	 34B	 21	 16	 19
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.25
	0.28 - 0.48
	0.51 - 0.61
	0.61 - 0.89
	0.89 - 1.09

	Project Name:	HOB
	Project Code:	HOB	Site ID:	H22	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_St	Smectite - X-Ray Diffraction
	XRD_C_Tc	Talc - Tourmaline - X-Ray Diffraction