Project Name:	SOR
	Project Code:	SOR	Site ID:	H84	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	C.G. Stephens	Locality:	91m E of Wattle Hill post office:
	Date Desc.:	04/02/54	Elevation:	 137 metres
	Map Ref.:	Sheet No. : 8412   1:100000	Rainfall:	640
	Northing/Long.:	147.633333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-42.7333333333333	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Basalt 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	8.8 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Black Vertosol     	Principal Profile Form:	Gn3.43
	ASC Confidence:	Great Soil Group:	Prairie soil
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.09 m	Very dark grey (10YR3/1-Moist); ; Light clay; , Granular; Moist; Weak consistence; 0-2%, Gravel, 
	coarse fragments; Diffuse change to - 
	A	0.09 - 0.14 m	Very dark grey (10YR3/1-Moist); ; Heavy clay; , Angular blocky; Moist; Moderately plastic; Normal 
	plasticity; Sharp change to - 
	B	0.14 - 0.25 m	Very dark greyish brown (2.5Y3/2-Moist); , 10YR31; Heavy clay; Massive grade of structure; 
	Moist; Moderately plastic; Normal plasticity; Diffuse change to - 
	B	0.25 - 0.38 m	Very dark greyish brown (2.5Y3/2-Moist); , 5Y41; Heavy clay; Massive grade of structure; Moist; 
	Moderately plastic; Normal plasticity; 2-10%, cobbly, 60-200mm, Basalt, coarse fragments; 
	Diffuse change to - 
	B	0.38 - 0.51 m	Dark greyish brown (2.5Y4/2-Moist); , 5Y41; Heavy clay; Massive grade of structure; Moist; 
	Moderately plastic; Normal plasticity; 0-2%, Basalt, coarse fragments; Diffuse change to - 
	B	0.51 - 0.63 m	Dark greyish brown (2.5Y4/3-Moist); ; Heavy clay; Massive grade of structure; Moist; Moderately 
	plastic; Normal plasticity; Diffuse change to - 
	B	0.66 - 0.76 m	Very dark greyish brown (2.5Y3/2-Moist); , 10YR56; Heavy clay; Massive grade of structure; 
	Moderately moist; Weak consistence; Diffuse change to - 
	BC	0.76 - 0.89 m	Olive brown (2.5Y4/4-Moist); , 5Y42; Moderately moist; 2-10%, Basalt, coarse fragments; Diffuse
	 change to - 
	C	1.29 - 1.42 m	Yellowish brown (10YR5/6-Moist); ; Moderately moist; Firm consistence; 
	Morphological Notes
	Observation Notes
	76-89CM MEALY DECOMPOSED BA WITH SOME CLAY:129-142CM MEALY W`D BA:51-63CM GREENISH (GLEYING) 
	FLECKS:MAYWA SERIES:       
	Site Notes
	PEMBROKE

	Project Name:	SOR
	Project Code:	SOR	Site ID:	H84	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	6.6A	 21.8H	 19.5	 0.32	 1.5	 10.6H	 63.1B
	 20E
	0.09 - 0.14	6.3A	 51C
	0.14 - 0.25	6.8A	 59C
	0.25 - 0.38	7.4A	 25.7H	 38.4	 0.22	 2.2	 12.3E	 79B
	0.38 - 0.51	7.9A
	0.51 - 0.63	7.9A	 59.5C
	0.66 - 0.76	8.3A
	0.76 - 0.89	8.6A
	1.29 - 1.42	6.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	 3.7D	 0.048D	 0.36A	 1	 2B	 25	 31	 37
	0.09 - 0.14	 3.1D	 0.04D	 0.293A
	0.14 - 0.25	 1.8D	 0.186A	 0	 1D	 18	 18	 56
	0.25 - 0.38	 0	 1D	 15	 17	 69
	0.38 - 0.51	<0.01A
	0.51 - 0.63	<0.01A	 0	<1B	 18	 26	 52
	0.66 - 0.76	<0.01A
	0.76 - 0.89	 0.03A
	1.29 - 1.42
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.14
	0.14 - 0.25
	0.25 - 0.38
	0.38 - 0.51
	0.51 - 0.63
	0.66 - 0.76
	0.76 - 0.89
	1.29 - 1.42

	Project Name:	SOR
	Project Code:	SOR	Site ID:	H84	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette