Project Name:	STM
	Project Code:	STM	Site ID:	H50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	C.G. Stephens	Locality:
	Date Desc.:	22/01/53	Elevation:	 244 metres
	Map Ref.:	Sheet No. : 8514   1:100000	Rainfall:	790
	Northing/Long.:	148.033333333333	Runoff:	Slow
	Easting/Lat.:	-41.5666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Pedal Aquic Vertosol     	Principal Profile Form:	Ug5.15
	ASC Confidence:	Great Soil Group:	Humic gley
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:	Low Strata - Sod grass, <0.25m, Closed or dense. *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Black (10YR2/1-Moist); ; Heavy clay; 20-50 mm, Angular blocky; Very strong consistence; 0-2%, 
	medium gravelly, 6-20mm, rounded, Gravel, coarse fragments; Diffuse change to - 
	A	0.1 - 0.23 m	Black (10YR2/1-Moist); ; Heavy clay; 20-50 mm, Angular blocky; Very strong consistence; 0-2%, 
	medium gravelly, 6-20mm, rounded, Gravel, coarse fragments; Diffuse change to - 
	A	0.24 - 0.36 m	Black (10YR2/1-Moist); ; Heavy clay; Firm consistence; Very few (0 - 2 %), Ferruginous, Fine (0 - 
	2 mm), Concretions; Diffuse change to - 
	A/B	0.36 - 0.48 m	Black (10YR2/1-Moist); , 5Y32; Heavy clay; Moist; Moderately plastic; Normal plasticity; Very few
	 (0 - 2 %), Ferruginous, Fine (0 - 2 mm), Concretions; Diffuse change to - 
	B	0.48 - 0.58 m	Black (10YR2/1-Moist); , 5Y52; , 5Y32; Heavy clay; , Prismatic; Fine, (0 - 5) mm crack; Moist; 
	Moderately plastic; Normal plasticity; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), 
	Concretions; Diffuse change to - 
	B/C	0.61 - 0.81 m	Olive grey (5Y5/2-Moist); , 10YR56; Heavy clay; , Prismatic; Fine, (0 - 5) mm crack; Moist; Weak 
	consistence; 0-2%, Gravel, coarse fragments; Diffuse change to - 
	C	0.84 - 1.07 m	Yellowish brown (10YR5/6-Moist); , 5Y62; Heavy clay; Wet; 50-90%, Gravel, coarse fragments; 
	Morphological Notes
	Observation Notes
	>117CM ON GRAVEL:48-107CM SLIGHT DIFFUSE LIME:24-48CM STRUCTURE IRREGULAR LUMPY WITH IRREGULAR 
	CLEAVAGE PLANES:         
	Site Notes
	CORNWALL

	Project Name:	STM
	Project Code:	STM	Site ID:	H50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.9A	 35.7H	 10.9	 0.59	 0.47	 10.2H	 67.76B
	 19.4E
	0.1 - 0.23	6.2A
	0.24 - 0.36	6.9A	 32.8H	 13	 0.38	 0.58	 4.7E	 51.11B
	0.36 - 0.48	7.7A
	0.48 - 0.58	7.8A	 24.3H	 7	 0.2	 0.6	 1.1E	 33.2B
	0.61 - 0.81	8.3A
	0.84 - 1.07	8.3A	 17.2K	 3.8	 0.12	 0.8	 22B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 6.05F	 0.016D	 0.541A	 1	 3B	 12	 21	 54
	 4.4D
	0.1 - 0.23	 4F	 0.38A
	 2.83D
	0.24 - 0.36	 1.7F	 0.006D	 0.154A	 0	 4B	 18	 17	 57
	 1.14D
	0.36 - 0.48
	0.48 - 0.58	 0.51F	 0.056A	 0	 11B	 30	 16	 43
	 0.37D
	0.61 - 0.81	 0.5A
	0.84 - 1.07	 49	 26B	 25	 14	 30
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.23
	0.24 - 0.36
	0.36 - 0.48
	0.48 - 0.58
	0.61 - 0.81
	0.84 - 1.07

	Project Name:	STM
	Project Code:	STM	Site ID:	H50	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6_DC	Organic carbon (%) - Dry combustion
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette