Project Name:	TYE
	Project Code:	TYE	Site ID:	H226	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	.7KM south east of National Park Railway Station:
	Date Desc.:	12/09/61	Elevation:	 250 metres
	Map Ref.:	Rainfall:	840
	Northing/Long.:	146.723611111111	Runoff:	Moderately rapid
	Easting/Lat.:	-42.6916666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Pm	Substrate Material:	Soil pit, 0.61 m deep,Mudstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3.5 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Natric Yellow Kurosol     	Principal Profile Form:	Dy2.61
	ASC Confidence:	Great Soil Group:	Grey-brown 
	All necessary analytical data are available.	podzolic soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Fern, , Sparse. *Species includes - None recorded
	Mid Strata - Tree, , Sparse. *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:	20-50%, , angular, Mudstone
	Profile Morphology
	A11	0 - 0.02 m	Black (10YR2/1-Moist); ; Loam; Weak grade of structure, <2 mm, Granular; Moist; Very weak 
	consistence; 2-10%, fine gravelly, 2-6mm, Mudstone, coarse fragments; ManyClear change to - 
	A12	0.02 - 0.09 m	Dark grey (10YR4/1-Moist); ; Fine sandy loam; Weak grade of structure, <2 mm, Granular; Moist; 
	Weak consistence; 10-20%, fine gravelly, 2-6mm, Mudstone, coarse fragments; Abundant, 
	coarse (>5mm) roots; Gradual, Irregular change to - 
	A1A2	0.09 - 0.11 m	Dark grey (10YR4/1-Moist); ; Fine sandy loam; 20-50%, coarse gravelly, 20-60mm, Mudstone, 
	coarse fragments; Common
	A2	0.11 - 0.18 m	Grey (10YR5/1-Moist); ; Fine sandy loam; Massive grade of structure; Few (<1 per 100mm2) Fine 
	(1-2mm) macropores, Moist; 20-50%, coarse gravelly, 20-60mm, Mudstone, coarse fragments; 
	CommonDiffuse change to - 
	A2B	0.18 - 0.3 m	Grey (10YR5/1-Moist); ; Fine sandy loam; Massive grade of structure; Few (<1 per 100mm2) Fine 
	(1-2mm) macropores, Moist; 50-90%, coarse gravelly, 20-60mm, Mudstone, coarse fragments; 
	CommonDiffuse change to - 
	B2	0.3 - 0.38 m	Light yellowish brown (10YR6/4-Moist); ; Heavy clay; Massive grade of structure; Moist; Weak 
	consistence; 50-90%, coarse gravelly, 20-60mm, Mudstone, coarse fragments; FewDiffuse 
	change to - 
	B2C	0.38 - 0.58 m	Light yellowish brown (10YR6/4-Moist); ; Heavy clay; Massive grade of structure; Moist; Weak 
	consistence; 50-90%, coarse gravelly, 20-60mm, Mudstone, coarse fragments; FewClear, Wavy 
	change to - 
	C	0.53 - 0.61 m	White (10YR8/1-Moist); , 10YR68; Fine sandy clay loam (Light); 
	Morphological Notes
	Observation Notes
	18-30CM POCKET OF CLAY IN CORNER:                                                                                       
	Site Notes
	ELLENDALE

	Project Name:	TYE
	Project Code:	TYE	Site ID:	H226	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)

	Project Name:	TYE
	Project Code:	TYE	Site ID:	H226	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	4.1A	 0.057A	 4.6H	 2.1	 0.64	 0.23	 35.4H	 51.1B
	 43.5E
	0.02 - 0.09	4A	 0.054A	 0.95H	 0.36	 0.3	 0.12	 13.1H	 20.1B
	 18.4E
	0.09 - 0.11	4A	 0.045A	 2
	0.11 - 0.18	4.2A	 0.033A	 0.3H	 0.09	 0.15	 0.07	 6.9H	 8.5B
	 7.9E
	0.18 - 0.3	4.4A	 0.03A
	0.3 - 0.38	4.8A	 0.039A	 0.24H	 0.75	 0.22	 0.24	 13.9H	 21.4B
	 19.9E
	0.38 - 0.58	5.1A	 0.027A
	0.53 - 0.61	5A	 0.024A	 0.22H	 1.7	 0.14	 0.22	 6.1H	 10.1B
	 7.8E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	 17.3D	 0.011D	 0.474A	 20	 6B	 34	 25	 12
	0.02 - 0.09	 4.19D	 0.004D	 0.123A	 26	 6B	 45	 32	 12
	0.09 - 0.11	 1.91D	 0.063A
	0.11 - 0.18	 0.98D	 0.041A	 28	 7D	 47	 33	 13
	0.18 - 0.3
	0.3 - 0.38	 49	 4D	 33	 21	 37
	0.38 - 0.58
	0.53 - 0.61	 0	 8D	 39	 30	 19
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.09
	0.09 - 0.11
	0.11 - 0.18
	0.18 - 0.3
	0.3 - 0.38
	0.38 - 0.58
	0.53 - 0.61

	Project Name:	TYE
	Project Code:	TYE	Site ID:	H226	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette