Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	9	Observation ID:	1
	Agency Name:	Conservation Commission of the Northern Territory
	Site Information
	Desc. By:	Locality:
	Date Desc.:	06/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 4966   1:100000	Rainfall:	No Data
	Northing/Long.:	8277770 AMG zone: 52	Runoff:	Slow
	Easting/Lat.:	647845  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Qt	Substrate Material:	Auger boring, 0.9 m deep,Slightly porous, 
	Alluvium 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	0 metres
	Elem. Type:	Levee	Slope Category:	No Data
	Slope:	0.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm, Cryptogam surface
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	53
	Haplic Eutrophic Brown Chromosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Clay-loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Chrysopogon fallax, Themeda triandra
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); , 0-0% ; Sandy clay loam (Light); Massive grade of structure; 
	Earthy fabric; Dry; Field pH 7 (Raupach); 
	A2	0.1 - 0.3 m	Dark reddish brown (5YR3/4-Moist); , 0-0% ; Clay loam; Massive grade of structure; Earthy fabric;
	 Dry; Field pH 7 (Raupach); 
	B21	0.3 - 0.6 m	Reddish brown (5YR4/4-Moist); , 0-0% ; Light medium clay; Moderate grade of structure; 
	Smooth-ped fabric; Dry; Field pH 7 (Raupach); 
	B22	0.6 - 0.9 m	Reddish brown (5YR4/4-Moist); , 0-0% ; Light medium clay; Moderate grade of structure; 
	Smooth-ped fabric; Dry; Field pH 7 (Raupach); 
	C	0.9 - 1.5 m	Reddish brown (5YR4/4-Moist); , 0-0% ; Light medium clay; Moderate grade of structure; 
	Smooth-ped fabric; Dry; Field pH 7 (Raupach); 
	Morphological Notes
	Observation Notes
	OLD ALLUVIAL TERRACE/ALP OF THE VIC RIVER.  DEEP STRUCTURED RED BROWN CLAY SUPPORTING AND DENSE
	 MIXED WOODLAND DOMINATED BY E.PRUIN OVER MIXED GRASSLAND.
	Site Notes

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	9	Observation ID:	1
	Agency Name:	Conservation Commission of the Northern Territory
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Bradshaw
	Project Code:	BRD	Site ID:	9	Observation ID:	1
	Agency Name:	Conservation Commission of the Northern Territory
	Laboratory Analyses Completed for this profile