Project Name:	Soil Investigation - Douglas Daly Carbon Water Study
	Project Code:	DDCWS	Site ID:	5	Observation ID:	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Site Information
	Desc. By:	Locality:
	Date Desc.:	14/09/09	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	131.739968	Runoff:	Slow
	Easting/Lat.:	-13.767625  Datum: GDA94	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Yellow Chromosol Very thick Moderately 	Principal Profile Form:	N/A
	gravelly Sandy  Deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.09 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Massive grade of structure; Earthy fabric; Field pH 6.2 (pH
	 meter); 
	A21e	0.09 - 0.42 m	Brownish yellow (10YR6/6-Moist); ; Sand; Massive grade of structure; Earthy fabric; Field pH 5.8 (pH 
	meter); 
	A22e	0.42 - 0.7 m	Brownish yellow (10YR6/6-Moist); ; Sand; Massive grade of structure; Earthy fabric; Field pH 6.1 (pH 
	meter); 
	B21	0.7 - 1 m	Brownish yellow (10YR6/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Field pH 6 (pH 
	meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Soil Investigation - Douglas Daly Carbon Water Study
	Project Code:	DDCWS	Site ID:	5	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.9C	0.018A	0.37H	0.16	0.07	0.06	0.15J
	6.2A
	0.1 - 0.2	4.7C	<0.01A	0.12H	0.13	0.06	0.05	0.26J
	5.8A
	0.2 - 0.3	4.9C	<0.01A	0.18H	0.22	0.06	0.05	0.11J
	5.8A
	0.5 - 0.6	5.5C	0.022A	0.1H	0.48	0.09	0.06	0.09J
	6.1A
	0.8 - 0.9	4.9C	<0.01A	0.12H	0.79	0.12	0.07	0.08J
	6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.63A	2J	0.03D	26	75.1A	14.3	5.8	4.8
	89.4G
	0.1 - 0.2	0.33A	2J	0.02D	22	81.8A	8.4	3.9	5.9
	90.2G
	0.2 - 0.3	0.22A	2J	0.04D	28	72.4A	14.1	7.8	5.8
	86.5G
	0.5 - 0.6	0.1A	2J	<0.01D	43	68.4A	16	4.9	10.7
	84.5G
	0.8 - 0.9	0.08A	2J	0.03D	77	61.6A	19.7	7.5	11.2
	81.3G
	Laboratory Analyses Completed for this profile
	10D1	Potassium chloride - 40 sulfur (KCl-40)-S
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	9B1	Bicarbonate-extractable phosphorus - manual colour
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_S	Sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)