Project Name:	Soil Investigation - NT Agriculture Association, Douglas Daly
	Project Code:	MNROO	Site ID:	3	Observation ID:	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Site Information
	Desc. By:	Locality:
	Date Desc.:	19/08/10	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	131.39684	Runoff:	Slow
	Easting/Lat.:	-13.727756  Datum: GDA94	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol Medium Non-gravelly Clay-	Principal Profile Form:	N/A
	loamy  Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1p	0 - 0.1 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Field pH 8.2 
	(pH meter); 
	B1p	0.1 - 0.17 m	Dusky red (2.5YR3/2-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Field pH 7.4 (pH 
	meter); 
	B21	0.17 - 0.8 m	Dark reddish brown (2.5YR3/4-Moist); ; Medium clay; Massive grade of structure; Earthy fabric; Field pH
	 7.2 (pH meter); 
	B22	0.8 - 1.2 m	Dusky red (10R3/4-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Field pH 6.6 (pH 
	meter); 
	B23	1.2 - 1.9 m	Dusky red (10R3/4-Moist); Dark red (10R3/6-Moist); ; Medium heavy clay; Massive grade of structure; 
	Earthy fabric; Field pH 6.8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Soil Investigation - NT Agriculture Association, Douglas Daly
	Project Code:	MNROO	Site ID:	3	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.1C	0.113A	15.72H	3.09	0.85	0.07	0.001J
	8.2A
	0.1 - 0.2	6.9C	0.044A	9H	1.77	0.46	0.07	0.001J
	7.4A
	0.2 - 0.3	6.8C	0.04A	6.34H	1.38	0.36	0.05	0.001J
	7.2A
	0.5 - 0.6	6.5C	0.02A	4.83H	0.53	0.28	0.06	0.001J
	7.2A
	0.8 - 0.9	6C	0.013A	4.51H	0.47	0.24	0.06	0.001J
	6.6A
	1.1 - 1.2	6.2C	0.021A	4.7H	0.59	0.28	0.04	0.001J
	6.6A
	1.4 - 1.5	6.2C	0.014A	5H	0.74	0.29	0.04	0.001J
	6.8A
	1.7 - 1.8	6.2C	0.018A	5.4H	0.88	0.36	0.04	0.001J
	6.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	2.01A	72J	0.2D	1	18.6A	26.4	22.2	32.8
	44.9G
	0.1 - 0.2	0.91A	9J	0.1D	0	14.3A	19	27.1	39.6
	33.3G
	0.2 - 0.3	0.62A	5J	0.08D	0	11A	24.3	26.9	37.8
	35.3G
	0.5 - 0.6	0.32A	2J	0.06D	1	9.2A	16.7	12.2	61.9
	25.9G
	0.8 - 0.9	0.19A	3J	0.06D	2	11A	17.9	15.7	55.4
	28.8G
	1.1 - 1.2	0.13A	6J	0.03D	3	9.9A	13.5	11.4	65.2
	23.4G
	1.4 - 1.5	0.1A	4J	0.04D	1	7.9A	10	17.8	64.3
	17.9G
	1.7 - 1.8	<0.05A	2J	0.04D	1	5.6A	10.6	21	62.8
	16.2G
	Laboratory Analyses Completed for this profile
	10D1	Potassium chloride - 40 sulfur (KCl-40)-S
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	18A1	Bicarbonate-extractable potassium

	Project Name:	Soil Investigation - NT Agriculture Association, Douglas Daly
	Project Code:	MNROO	Site ID:	3	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	9B1	Bicarbonate-extractable phosphorus - manual colour
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_S	Sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)