Project Name:	Land Resources of the Victoria River District representative Soil Sampling 2011
	Project Code:	VRD_11	Site ID:	10	Observation ID:	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Site Information
	Desc. By:	Locality:
	Date Desc.:	30/05/11	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	129.598509	Runoff:	No runoff
	Easting/Lat.:	-17.841714  Datum: GDA94	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Brown Vertosol Non-gravelly Medium fine 	Principal Profile Form:	N/A
	Very fine  
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1	0 - 0.1 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; Strong grade of structure; Smooth-ped fabric; Field 
	pH 6.6 (pH meter); 
	B21	0.1 - 1.1 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Strong grade of structure; Smooth-ped 
	fabric; Field pH 8.1 (pH meter); 
	B22	1.1 - 1.5 m	Dark yellowish brown (10YR4/4-Moist); ; Medium heavy clay; Strong grade of structure; Smooth-ped 
	fabric; Field pH 8.3 (pH meter); 
	B23	1.5 - 2.05 m	Dark yellowish brown (10YR4/4-Moist); ; Heavy clay; Strong grade of structure; Smooth-ped fabric; Field 
	pH 7.8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Land Resources of the Victoria River District representative Soil Sampling 2011
	Project Code:	VRD_11	Site ID:	10	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6C	0.101A	15.1H	6.34	0.85	0.09	0.001J
	6.6A
	0.1 - 0.2	6.1C	0.025A	16.15H	5.37	0.72	0.17	0.001J
	8.1A
	0.2 - 0.3	6.4C	0.027A	16.73H	4.41	0.68	0.31	0.001J
	8.1A
	0.5 - 0.6	6.7C	0.034A	16.95H	3.69	0.72	0.71	0.001J
	8.1A
	0.8 - 0.9	7C	0.088A	17.38H	5.26	0.54	1.25	0.001J
	8.1A
	1.1 - 1.2	7.3C	0.138A	17.77H	4.05	0.6	1.81	0.001J
	8.3A
	1.4 - 1.5	7.6C	0.289A	19.19H	2.48	0.63	2.19	0.001J
	8.3A
	1.7 - 1.8	7.6C	1.249A	20.02H	1.86	0.65	2.37	0.001J
	7.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.37A	<2J	0.05D	1.49	0	3.14A	31.7	13.43	51.76
	34.84G
	0.1 - 0.2	0.27A	<2J	0.1D	1.46	1	3.22A	24.1	16.71	55.98
	27.32G
	0.2 - 0.3	0.27A	<2J	0.04D	1.48	3.68A	26.3	14.02	56.02
	29.98G
	0.5 - 0.6	0.29A	<2J	0.01D	1.56	1	3.52A	27	10.92	58.51
	30.52G
	0.8 - 0.9	0.26A	<2J	0.03D	1.57	3.83A	28.1	11.02	57.04
	31.93G
	1.1 - 1.2	0.23A	<2J	0.07D	1.64	2.2A	30.6	15.52	51.69
	32.8G
	1.4 - 1.5	0.18A	<2J	<0.01D	1.56	3.26A	24.7	13.82	58.19
	27.96G
	1.7 - 1.8	0.11A	<2J	0.05D	1.52	19.53A	55.3	16.78	8.34
	74.83G
	Laboratory Analyses Completed for this profile
	10D1	Potassium chloride - 40 sulfur (KCl-40)-S
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts

	Project Name:	Land Resources of the Victoria River District representative Soil Sampling 2011
	Project Code:	VRD_11	Site ID:	10	Observation 	1
	Agency Name:	NT Natural Resources, Environment and the Arts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	9B1	Bicarbonate-extractable phosphorus - manual colour
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_S	Sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)
	P3A1	Bulk density - g/cm3