Project Name:	AS1
	Project Code:	AS1	Site ID:	NT25	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	E.A. Jackson	Locality:
	Date Desc.:	05/09/58	Elevation:	 457 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	133.455833333333	Runoff:	Moderately rapid
	Easting/Lat.:	-24.3780555555556	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling plains <9m 10-32%	Pattern Type:	Pediment
	Morph. Type:	Crest	Relief:	6 metres
	Elem. Type:	Pediment	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Eutrophic Red Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Shrub, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	; Loamy sand; Weak grade of structure, Platy; Weak consistence; 50-90%, stony, 200-600mm, 
	Quartz, coarse fragments; Abrupt change to - 
	0.05 - 0.08 m	Pink (5YR7/4-Moist); ; Clay loam; Massive grade of structure; Firm consistence; 2-10%, fine 
	gravelly, 2-6mm, Gravel, coarse fragments; Diffuse change to - 
	0.08 - 0.15 m	Light red (2.5YR7/6-Moist); ; Medium clay; Weak grade of structure, Prismatic; Strong grade of 
	structure, 10-20 mm, Angular blocky; Very firm consistence; 2-10%, fine gravelly, 2-6mm, Slate, 
	coarse fragments; Diffuse change to - 
	0.15 - 0.26 m	Red (2.5YR4/6-Moist); , 2.5YR46, 0-2% ; , 0-2% ; Medium clay; Moderate grade of structure, 20-
	50 mm, Angular blocky; Firm consistence; 2-10%, fine gravelly, 2-6mm, Gravel, coarse 
	fragments; Common, fine (1-2mm) roots; Clear change to - 
	0.26 - 0.43 m	, 2-10% ; , 2-10% ; Clay loam; Weak grade of structure, 10-20 mm, Angular blocky; Firm 
	consistence; 20-50%, Slate, coarse fragments; Very few (0 - 2 %), Gypseous, , Soft 
	segregations; Clear change to - 
	0.48 - 0.78 m	; 50-90%, Slate, coarse fragments; Many (20 - 50 %), Gypseous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	MODERATE PAVEMENT OF QUARTZITE GIBBERS 1-5CM: SLATY FINE GRAVEL:                                                        
	Site Notes
	ALICE SPRINGS

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT25	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.1H	 0.014C	 2.2K	 2.4	 0.32	 0.07
	0.05 - 0.08	6.9H	 0.018C
	0.08 - 0.15	6.9H	 0.049C	 6.7K	 7.8	 0.63	 0.91
	0.15 - 0.26	7.7H	 0.082C
	0.26 - 0.43	7.8H
	0.48 - 0.78	7.9H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.21E	 0.029F	 0.033B	 0.25B	 45	 19C	 54	 17	 11
	0.05 - 0.08	 0.026F	 0.034B	 0.4B	 11	 12C	 45	 23	 22
	0.08 - 0.15	 0.045B	 4	 8C	 31	 17	 44
	0.15 - 0.26
	0.26 - 0.43	 0.03C	 12	 9C	 31	 29	 34
	0.48 - 0.78	 0.17C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.08
	0.08 - 0.15
	0.15 - 0.26
	0.26 - 0.43
	0.48 - 0.78

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT25	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded