Project Name:	AS1
	Project Code:	AS1	Site ID:	NT35	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	E.A. Jackson	Locality:
	Date Desc.:	07/09/58	Elevation:	 457 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	134.820555555556	Runoff:	Slow
	Easting/Lat.:	-24.1086111111111	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Sand plain
	1-3%
	Morph. Type:	No Data	Relief:	100 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Calcareous red 
	Analytical data are incomplete but reasonable confidence.	earth
	Site Disturbance:
	Vegetation:
	Mid Strata - Shrub, , . *Species includes - Salsola kali
	Tall Strata - Shrub, , . *Species includes - Acacia georginae
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Yellowish red (5YR5/6-Moist); ; Loam; Weak grade of structure, Platy; Diffuse change to - 
	0.08 - 0.15 m	Yellowish red (5YR5/6-Moist); ; Loam; Weak grade of structure, 10-20 mm, Angular blocky; 
	Diffuse change to - 
	0.15 - 0.4 m	Yellowish red (5YR4/6-Moist); ; Loam; Weak grade of structure, 10-20 mm, Angular blocky; Very 
	few (0 - 2 %), Calcareous, , Concretions; 
	0.4 - 0.61 m	Red (2.5YR4/6-Moist); ; Clay loam; Few (2 - 10 %), Calcareous, , Soft segregations; 
	0.61 - 0.96 m	Red (2.5YR4/6-Moist); ; Clay loam; Common (10 - 20 %), Calcareous, , Soft segregations; 
	0.96 - 1.32 m	Red (2.5YR4/6-Moist); ; Clay loam; Many (20 - 50 %), Calcareous, , Soft segregations; 
	1.32 - 1.6 m	Red (2.5YR4/6-Moist); ; Clay loam; Many (20 - 50 %), Calcareous, , Concretions; 
	Morphological Notes
	Observation Notes
	Site Notes
	ALICE SPRINGS

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT35	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.6H	 0.027C
	0.08 - 0.15	8.7H	 0.021C
	0.15 - 0.4	8.8H	 0.022C	 7.6K	 3.4	 1.4	 0.05
	0.4 - 0.61	8.9H	 0.033C
	0.61 - 0.96	9H	 0.035C
	0.96 - 1.32	9.1H	 0.035C
	1.32 - 1.6	9.1H	 0.046C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.27C	 0.03F	 0.046B	 0.52B	 6C	 68	 10	 13
	0.08 - 0.15	 0.05C	 0.031B
	0.15 - 0.4	 0.04C	 6C	 63	 6	 22
	0.4 - 0.61	 0.65C	 6C	 59	 5	 26
	0.61 - 0.96	 8.1C
	0.96 - 1.32	 11C
	1.32 - 1.6	 10C	 12	 3C	 45	 8	 24
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.15
	0.15 - 0.4
	0.4 - 0.61
	0.61 - 0.96
	0.96 - 1.32
	1.32 - 1.6

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT35	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded