Project Name:	AS1
	Project Code:	AS1	Site ID:	NT36	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	E.A. Jackson	Locality:
	Date Desc.:	28/08/58	Elevation:	 70 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	133.835277777778	Runoff:	Slow
	Easting/Lat.:	-23.46	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Hypercalcic Red Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Calcareous red 
	All necessary analytical data are available.	earth
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Shrub, , . *Species includes - Acacia aneura
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Red (2.5YR4/6-Moist); ; Sandy loam; Weak grade of structure, Platy; Weak consistence; Field 
	pH 5 (pH meter); 
	0.08 - 0.29 m	Red (10R5/6-Moist); ; Sandy medium clay; Massive grade of structure; Weak consistence; Field 
	pH 5.5 (pH meter); Few, medium (2-5mm) roots; Diffuse change to - 
	0.29 - 0.61 m	Red (10R4/6-Moist); ; Sandy medium clay; Massive grade of structure; Firm consistence; 2-10%,
	 Quartz, coarse fragments; Field pH 6 (pH meter); 
	0.61 - 0.89 m	Dark red (10R3/6-Moist); ; Sandy medium clay; Massive grade of structure; Very firm 
	consistence; 2-10%, Quartz, coarse fragments; Field pH 6 (pH meter); 
	0.89 - 1.19 m	Dark red (10R3/6-Moist); ; Sandy medium clay; Massive grade of structure; Very firm 
	consistence; 0-2%, medium gravelly, 6-20mm, Gravel, coarse fragments; Field pH 6.5 (pH 
	meter); 
	1.37 - 1.57 m	Red (10R4/6-Moist); ; Medium clay; Field pH 7 (pH meter); 
	1.57 - 1.83 m	Red (10R4/6-Moist); ; Medium clay; Few (2 - 10 %), Calcareous, , Concretions; Field pH 7 (pH 
	meter); 
	1.83 - 1.91 m	Red (10R4/6-Moist); ; Medium clay; Field pH 8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	ALICE SPRINGS

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT36	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08
	0.08 - 0.29
	0.29 - 0.61
	0.61 - 0.89
	0.89 - 1.19
	1.37 - 1.57
	1.57 - 1.83
	1.83 - 1.91
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.29
	0.29 - 0.61
	0.61 - 0.89
	0.89 - 1.19
	1.37 - 1.57
	1.57 - 1.83
	1.83 - 1.91
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.29
	0.29 - 0.61
	0.61 - 0.89
	0.89 - 1.19
	1.37 - 1.57
	1.57 - 1.83
	1.83 - 1.91

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT36	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile