Project Name:	AS1
	Project Code:	AS1	Site ID:	NT39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	E.A. Jackson	Locality:
	Date Desc.:	08/10/58	Elevation:	 732 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	134.424444444444	Runoff:	Slow
	Easting/Lat.:	-23	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Tall Strata - Shrub, , . *Species includes - Acacia aneura, Atalaya hemiglauca, Unknown species
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.01 m	; Clayey sand; Single grain grade of structure; Loose consistence; 20-50%, medium gravelly, 6-
	20mm, Gravel, coarse fragments; Sharp change to - 
	0.01 - 0.03 m	; Sandy loam; Massive grade of structure; Weak consistence; Diffuse change to - 
	0.03 - 0.25 m	; Sandy loam; Massive grade of structure; Firm consistence; Diffuse change to - 
	0.25 - 0.33 m	; Sandy clay loam; Massive grade of structure; Very firm consistence; 
	0.33 - 0.48 m	; Sandy medium clay; Very firm consistence; 2-10%, cobbly, 60-200mm, Gravel, coarse 
	fragments; 
	0.48 - 0.66 m	; Light clay; Massive grade of structure; Very firm consistence; 2-10%, Gravel, coarse fragments; 
	0.66 - 0.79 m	Dark red (2.5YR3/6-Moist); ; Sandy medium clay; 
	0.79 - 1.06 m	Red (2.5YR4/6-Moist); ; Sandy medium clay; Very firm consistence; 0-2%, Gravel, coarse 
	fragments; Field pH 7.5 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	ALICE SPRINGS

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01	7.4H	 0.011C
	0.01 - 0.03	7.1H	 0.017C	 2.7K	 1.9	 0.97	 0.03
	0.03 - 0.25	7.1H	 0.014C
	0.25 - 0.33	7.5H	 0.01C
	0.33 - 0.48	7.6H	 0.015C
	0.48 - 0.66	7.6H	 0.025C	 7K	 6.2	 1.1	 0.19
	0.66 - 0.79	7.6H	 0.025C
	0.79 - 1.06	8.4H	 0.014C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01	 0.012B
	0.01 - 0.03	 0.19E	 0.022F	 0.022B	 0.46B	 4	 49C	 34	 7	 9
	0.03 - 0.25
	0.25 - 0.33	 7	 44C	 33	 5	 16
	0.33 - 0.48
	0.48 - 0.66	 5	 37C	 6	 2	 32
	0.66 - 0.79
	0.79 - 1.06	 0.02C	 7	 36C	 32	 3	 27
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.03
	0.03 - 0.25
	0.25 - 0.33
	0.33 - 0.48
	0.48 - 0.66
	0.66 - 0.79
	0.79 - 1.06

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT39	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded