Project Name:	AS1
	Project Code:	AS1	Site ID:	NT41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	E.A. Jackson	Locality:
	Date Desc.:	09/10/58	Elevation:	 701 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	134.697777777778	Runoff:	Slow
	Easting/Lat.:	-23.3055555555556	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Regolithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Tall Strata - Shrub, , . *Species includes - Acacia aneura
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.04 m	Yellowish red (5YR5/6-Moist); ; Clay loam; , Platy; Weak consistence; 20-50%, Gravel, coarse 
	fragments; Very few (0 - 2 %), Calcareous, , Concretions; Diffuse change to - 
	0.04 - 0.23 m	Reddish brown (5YR5/4-Moist); ; Medium clay; Weak grade of structure, Prismatic; , Angular 
	blocky; Very firm consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Diffuse change 
	to - 
	0.23 - 0.43 m	Reddish brown (5YR5/4-Moist); ; Medium clay; Strong grade of structure, 50-100 mm, Angular 
	blocky; Medium, (5 - 10) mm crack; Very firm consistence; Common (10 - 20 %), Calcareous, , 
	Concretions; 
	0.43 - 0.64 m	Reddish brown (5YR5/4-Moist); ; Clay loam; Many (20 - 50 %), Calcareous, , Soft segregations; 
	0.64 - 0.89 m	Reddish brown (5YR5/4-Moist); ; Clay loam; Few (2 - 10 %), Calcareous, , Soft segregations; 
	Common (10 - 20 %), Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes
	ALICE SPRINGS

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	8.8H	 0.032C
	0.04 - 0.23	9H	 0.044C
	0.23 - 0.43	8.5H	 0.27C
	0.43 - 0.64	8.4H	 0.62C
	0.64 - 0.89	8.6H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 1.2C	 0.42E	 0.015F	 0.043B	 0.36B	 23C	 30	 11	 31
	0.04 - 0.23	 3.8C	 0.04B	 3	 16C	 24	 6	 46
	0.23 - 0.43	 7.6C
	0.43 - 0.64	 18C
	0.64 - 0.89	 21C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.23
	0.23 - 0.43
	0.43 - 0.64
	0.64 - 0.89

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded