Project Name:	AS1
	Project Code:	AS1	Site ID:	NT51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	E.A. Jackson	Locality:	CALC. SHALE OR LIMESTONE OUTCROPPING AT 
	SURFACE: MUCH DEAD TIMBER:
	Date Desc.:	03/02/59	Elevation:	 457 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	134.075277777778	Runoff:	Moderately rapid
	Easting/Lat.:	-24.4169444444445	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Pediment
	Morph. Type:	No Data	Relief:	3 metres
	Elem. Type:	Pediment	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Paralithic Hypercalcic Calcarosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Red calcareous 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:
	Vegetation:
	Mid Strata - Shrub, , . *Species includes - Acacia aneura
	Tall Strata - Tree, , . *Species includes - Atalaya hemiglauca
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.09 m	Reddish brown (5YR5/4-Moist); ; Loam; Weak grade of structure, Platy; , Angular blocky; Weak 
	consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Sharp change to - 
	0.09 - 0.15 m	Reddish brown (5YR5/4-Moist); ; Loam; Weak grade of structure, 20-50 mm, Angular blocky; 
	Firm consistence; Common (10 - 20 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.15 - 0.27 m	Light reddish brown (5YR6/4-Moist); ; Clay loam; Weak grade of structure, Angular blocky; Firm 
	consistence; Many (20 - 50 %), Calcareous, , Soft segregations; Diffuse change to - 
	0.27 - 0.37 m	Light reddish brown (5YR6/4-Moist); ; Clay loam; 5-10 mm, Angular blocky; Very firm 
	consistence; 10-20%, stony, 200-600mm, Gravel, coarse fragments; Many (20 - 50 %), 
	Calcareous, , Soft segregations; Diffuse change to - 
	0.37 - 0.51 m	; Clay loam; Many (20 - 50 %), Calcareous, , Soft segregations; 
	Morphological Notes
	Observation Notes
	Site Notes
	ALICE SPRINGS

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	9.1H	 0.029C
	0.09 - 0.15	9.1H	 0.031C
	0.15 - 0.27	9.1H	 0.029C
	0.27 - 0.37	9.1H	 0.03C	 2K	 0.6	 0.21	 0.6
	0.37 - 0.51	9H	 0.033C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	 7.8C	 0.48E	 0.025F	 0.055B	 0.51B	 2	 11C	 58	 8	 14
	0.09 - 0.15	 12C	 2	 9C	 51	 7	 17
	0.15 - 0.27	 20C	 5	 7C	 46	 7	 17
	0.27 - 0.37	 33C
	0.37 - 0.51	 31C	 0.015F	 0.69B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.15
	0.15 - 0.27
	0.27 - 0.37
	0.37 - 0.51

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT51	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded