Project Name:	AS1
	Project Code:	AS1	Site ID:	NT64	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	E.A. Jackson	Locality:
	Date Desc.:	25/09/59	Elevation:	 762 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	132.075555555556	Runoff:	Moderately rapid
	Easting/Lat.:	-23.7813888888889	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	0 metres
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.08 m	Reddish brown (2.5YR5/4-Moist); ; Sand; Massive grade of structure; Very weak consistence; 
	0.08 - 0.3 m	Reddish brown (2.5YR5/4-Moist); ; Sand; Massive grade of structure; Very weak consistence; 
	0.3 - 0.61 m	Red (10R5/6-Moist); ; Clayey sand; Massive grade of structure; Very weak consistence; 
	0.61 - 0.91 m	Red (10R5/6-Moist); ; Clayey sand; Massive grade of structure; Very weak consistence; 0-2%, 
	fine gravelly, 2-6mm, Gravel, coarse fragments; 
	0.91 - 1.04 m	Red (2.5YR5/8-Moist); ; Clayey sand; Massive grade of structure; Weak consistence; 2-10%, 
	Gravel, coarse fragments; Sharp change to - 
	1.04 - 1.24 m	; Clayey sand; Weak grade of structure, Platy; Weak consistence; 20-50%, Gravel, coarse 
	fragments; Sharp change to - 
	1.24 - 1.29 m	; Clayey sand; Massive grade of structure; Strong consistence; 2-10%, Gravel, coarse 
	fragments; Diffuse change to - 
	1.29 - 1.4 m	Brownish yellow (10YR6/6-Moist); , 10YR36; Sandy medium clay; Massive grade of structure; 
	Strong consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	ALICE SPRINGS

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT64	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.3H	 0.004C	 1.1K	 0.6	 0.2	 0.02
	0.08 - 0.3	5.9H	 0.006C
	0.3 - 0.61	5.8H	 0.005C
	0.61 - 0.91	5.6H	 0.006C
	0.91 - 1.04	5.7H	 0.005C
	1.04 - 1.24	6H	 0.01C
	1.24 - 1.29	6.1H	 0.02C
	1.29 - 1.4	6.7H	 0.034C	 2.9K	 5.3	 0.77	 0.67
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 0.19E	 0.007F	 0.17B	 0.09B	 50C	 42	 0	 8
	0.08 - 0.3
	0.3 - 0.61
	0.61 - 0.91
	0.91 - 1.04
	1.04 - 1.24
	1.24 - 1.29
	1.29 - 1.4	 38C	 30	 1	 31
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.3
	0.3 - 0.61
	0.61 - 0.91
	0.91 - 1.04
	1.04 - 1.24
	1.24 - 1.29
	1.29 - 1.4

	Project Name:	AS1
	Project Code:	AS1	Site ID:	NT64	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_NR	Total element - K(%) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded