Project Name:	CAE
	Project Code:	CAE	Site ID:	A391	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	E.A. Jackson	Locality:
	Date Desc.:	19/06/56	Elevation:	 610 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	133.966666666667	Runoff:	Slow
	Easting/Lat.:	-23.7666666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	1 metres
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Alluvial soil
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.14 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Very weak 
	consistence; 2-10%, fine gravelly, 2-6mm, Other, coarse fragments; Sharp change to - 
	0.14 - 0.2 m	Yellowish red (5YR4/6-Moist); ; Fine sandy loam; Massive grade of structure; Firm consistence; 
	Abrupt change to - 
	0.2 - 0.45 m	Reddish brown (5YR4/4-Moist); ; Sandy loam; Massive grade of structure; Firm consistence; 2-
	10%, fine gravelly, 2-6mm, Other, coarse fragments; Diffuse change to - 
	0.45 - 0.75 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Firm consistence;
	 0-2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Abrupt change to - 
	0.75 - 0.88 m	Yellowish red (5YR4/8-Moist); ; Clay loam, fine sandy; Massive grade of structure; Firm 
	consistence; 2-10%, fine gravelly, 2-6mm, Other, coarse fragments; 
	1.08 - 1.36 m	; Sandy loam; 0-2%, coarse gravelly, 20-60mm, Other, coarse fragments; 
	1.36 - 1.65 m	; Sand; 2-10%, medium gravelly, 6-20mm, Other, coarse fragments; 
	1.8 - 1.95 m	; Clay loam, fine sandy; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	CAE
	Project Code:	CAE	Site ID:	A391	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.14	7.9H	 0.024C	 3.8K	 1.1	 17	 0.15
	 1.2
	0.14 - 0.2	7.8H	 0.019C	 8.2K	 2	 24	 0.14
	 1.5
	0.2 - 0.45	8.1H	 0.009C
	0.45 - 0.75	8.1H	 0.015C
	0.75 - 0.88	7.8H	 0.025C	 11.7K	 2.9	 1.1	 0.48
	1.08 - 1.36	8.1H	 0.015C
	1.36 - 1.65	8.2H	 0.01C
	1.83 - 1.98	8.3H	 0.027C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.14	 0.01C	 0.042F	 0.028B	 6	 36C	 51	 6	 7
	0.14 - 0.2	 0.01C	 0.045F	 0.05B	 17C	 57	 17	 10
	0.2 - 0.45	 0.01C
	0.45 - 0.75	 0.01C
	0.75 - 0.88	 0.01C	 17C	 38	 28	 18
	1.08 - 1.36	 0.01C
	1.36 - 1.65	 0.01C
	1.83 - 1.98	 0.03C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.14
	0.14 - 0.2
	0.2 - 0.45
	0.45 - 0.75
	0.75 - 0.88
	1.08 - 1.36
	1.36 - 1.65
	1.83 - 1.98

	Project Name:	CAE
	Project Code:	CAE	Site ID:	A391	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded