Project Name:	CAS
	Project Code:	CAS	Site ID:	NT86	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	W.H. Litchfield	Locality:	THIS PROFILE IS SITUATED IN A SLIGHT 
	DEPRESSION
	Date Desc.:	06/07/61	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	133.869166666667	Runoff:	No Data
	Easting/Lat.:	-23.7730555555556	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.3 m	Dark reddish brown (5YR3/3-Moist); Brown (7.5YR5/3-Dry); ; Fine sand (Light); Single grain grade
	 of structure; Very firm consistence; Moderately plastic; 
	0.3 - 0.48 m	Dark reddish brown (5YR3/4-Moist); Brown (7.5YR5/4-Dry); ; Loamy fine sand (Light); Firm 
	consistence; Very plastic; 
	0.48 - 0.74 m	Dark reddish brown (5YR3/4-Moist); Brown (7.5YR5/4-Dry); ; Loamy sand; Very firm consistence; 
	Very plastic; 0-2%, coarse gravelly, 20-60mm, Sand, coarse fragments; 
	0.74 - 0.89 m	Dark reddish brown (5YR3/4-Moist); Reddish brown (5YR4/4-Dry); ; Sandy medium clay (Light); 
	Single grain grade of structure; Strong consistence; 0-2%, coarse gravelly, 20-60mm, Sand, 
	coarse fragments; 
	0.89 - 1.37 m	; Sandy medium clay (Light); Single grain grade of structure; Strong consistence; 10-20%, 
	coarse gravelly, 20-60mm, Sand, coarse fragments; Diffuse change to - 
	1.37 - 1.47 m	; 
	1.47 - 1.78 m	Brown (7.5YR4/4-Moist); Light brown (7.5YR6/4-Dry); ; Fine sandy loam (Light); Single grain 
	grade of structure; Weak consistence; Very plastic; Many (20 - 50 %), Calcareous, , Soft 
	segregations; 
	2.77 - 2.94 m	Dark red (2.5YR3/6-Moist); ; Loamy sand; Single grain grade of structure; Sharp change to - 
	2.94 - 3.12 m	Dark red (10R3/6-Moist); ; Clay loam, sandy; 20-50%, coarse gravelly, 20-60mm, Sand, coarse 
	fragments; Sharp change to - 
	3.12 - 3.25 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy clay loam; Single grain grade of structure; 
	Strong consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	3.25 - 3.45 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy clay loam; Single grain grade of structure; 
	Strong consistence; Few (2 - 10 %), Calcareous, , Soft segregations; 
	3.45 - 3.75 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy clay loam; Single grain grade of structure; 
	Few (2 - 10 %), Calcareous, , Soft segregations; 
	3.75 - 4.05 m	Dark red (10R3/6-Moist); Red (10R4/6-Dry); ; Sandy clay loam; Single grain grade of structure; 
	Strong consistence; Few (2 - 10 %), Calcareous, , Soft segregations; Gradual change to - 

	Project Name:	CAS
	Project Code:	CAS	Site ID:	NT86	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	4.05 - 4.48 m	; Clay loam, sandy; Firm consistence; 20-50%, medium gravelly, 6-20mm, Sand, coarse 
	fragments; 
	Morphological Notes
	KO1
	KO2
	K11
	K2
	K12
	K1K2
	K21
	K11
	K31
	K32
	K32
	K32
	K32
	K33
	Observation Notes
	COVERED WITH A SHEET OF AMOONGUNA ALLUVIUM:                                                                             
	Site Notes
	EMILY PLAIN 1

	Project Name:	CAS
	Project Code:	CAS	Site ID:	NT86	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.3	7.7H	 0.028C
	0.3 - 0.48	7.8H	 0.036C
	0.48 - 0.74	7.7H	 0.024C
	0.74 - 0.89	8H	 0.012C
	0.89 - 1.37	7.8H	 0.012C
	1.37 - 1.47	8.1H	 0.01C
	1.47 - 1.78	8.6H	 0.031C
	2.77 - 2.94	8.9H	 0.035C
	2.94 - 3.12	8.8H	 0.012C
	3.12 - 3.25	8.8H	 0.013C
	3.25 - 3.45	8.7H	 0.019C
	3.45 - 3.75	8.9H	 0.025C
	3.75 - 4.05	8.9H	 0.026C
	4.05 - 4.48	8.9H	 0.016C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.3	 0.045B	 0	 7C	 60	 20	 12
	0.3 - 0.48	 0.034B	 0	 9C	 66	 11	 13
	0.48 - 0.74
	0.74 - 0.89	 0.01C	 1	 25C	 45	 11	 19
	0.89 - 1.37	 0.01C	 8	 24C	 46	 11	 16
	1.37 - 1.47	 0.01C	 0.019B	 5	 20C	 46	 18	 15
	1.47 - 1.78	 0.67C	 0.022B
	2.77 - 2.94	 0.11C	 0.01B	 0	 26C	 44	 15	 13
	2.94 - 3.12	 0.01C	 0.006B	 1	 47C	 40	 4	 9
	3.12 - 3.25	 0.01C	 0	 47C	 30	 3	 17
	3.25 - 3.45	 0.02C	 0	 43C	 28	 4	 23
	3.45 - 3.75	 0.06C	 0	 44C	 30	 6	 17
	3.75 - 4.05	 0.1C	 0	 52C	 24	 5	 14
	4.05 - 4.48	 0.04C	 0	 60C	 23	 5	 10
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.3
	0.3 - 0.48
	0.48 - 0.74
	0.74 - 0.89
	0.89 - 1.37
	1.37 - 1.47
	1.47 - 1.78
	2.77 - 2.94
	2.94 - 3.12
	3.12 - 3.25
	3.25 - 3.45
	3.45 - 3.75
	3.75 - 4.05

	Project Name:	CAS
	Project Code:	CAS	Site ID:	NT86	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	4.05 - 4.48

	Project Name:	CAS
	Project Code:	CAS	Site ID:	NT86	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded