Project Name:	CAS
	Project Code:	CAS	Site ID:	NT89	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Site Information
	Desc. By:	W.H. Litchfield	Locality:	ON FLOODPLAIN OF HARRY CREEK
	Date Desc.:	18/07/61	Elevation:	 720 metres
	Map Ref.:	Rainfall:	0
	Northing/Long.:	133.728055555556	Runoff:	Slow
	Easting/Lat.:	-23.2747222222222	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Flood plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Tall Strata - Shrub, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.4 m	Reddish brown (5YR4/4-Moist); ; Silty medium clay; Weak grade of structure, 2-5 mm, 
	Polyhedral; Very firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Diffuse
	 change to - 
	0.4 - 0.8 m	Reddish brown (5YR4/4-Moist); ; Silty medium clay; Moderate grade of structure, 20-50 mm, 
	Polyhedral; Strong consistence; 0-2%, medium gravelly, 6-20mm, Gravel, coarse fragments; 
	Diffuse change to - 
	0.8 - 1 m	Reddish yellow (7.5YR6/6-Moist); ; Silty clay loam; Single grain grade of structure; Very firm 
	consistence; Clear change to - 
	1 - 1.18 m	Reddish yellow (7.5YR6/6-Moist); ; Silty clay loam; Single grain grade of structure; Firm 
	consistence; Very few (0 - 2 %), Calcareous, , Soft segregations; Clear change to - 
	1.18 - 1.33 m	Brown (7.5YR5/4-Moist); ; Loam; Single grain grade of structure; Weak consistence; Very few (0 
	- 2 %), Calcareous, , Soft segregations; Sharp change to - 
	1.33 - 1.41 m	Brown (7.5YR5/4-Moist); ; Loamy sand; Single grain grade of structure; Firm consistence; Very 
	few (0 - 2 %), Calcareous, , Soft segregations; Sharp change to - 
	1.41 - 1.51 m	Light reddish brown (5YR6/4-Moist); ; Silty clay loam; Single grain grade of structure; Very firm 
	consistence; Very few (0 - 2 %), Calcareous, , Soft segregations; Clear change to - 
	1.51 - 1.66 m	Reddish brown (5YR5/4-Moist); ; Silty clay loam; 5-10 mm, Angular blocky; Strong consistence; 
	20-50%, Sand, coarse fragments; Very few (0 - 2 %), Calcareous, , Soft segregations; 
	1.91 - 2.21 m	Reddish brown (5YR5/4-Moist); ; Silty clay loam; 5-10 mm, Angular blocky; Strong consistence; 
	20-50%, Sand, coarse fragments; Very few (0 - 2 %), Calcareous, , Soft segregations; 
	2.21 - 2.57 m	Reddish brown (5YR5/4-Moist); ; Silty clay loam; 5-10 mm, Angular blocky; Strong consistence; 
	Very few (0 - 2 %), Calcareous, , Soft segregations; Sharp change to - 
	2.57 - 2.62 m	Yellowish red (5YR4/6-Moist); ; Coarse sandy medium clay; Strong consistence; Very few (0 - 2 
	%), Calcareous, , Soft segregations; 
	2.62 - 2.7 m	Yellowish red (5YR4/6-Moist); ; Clayey sand; 10-20 mm, Angular blocky; Strong consistence; 
	Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Soft segregations; 

	Project Name:	CAS
	Project Code:	CAS	Site ID:	NT89	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	2.73 - 2.99 m	Reddish brown (5YR5/4-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Strong consistence; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Soft 
	segregations; 
	2.99 - 3.24 m	Reddish brown (5YR5/4-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Angular blocky; Strong consistence; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Soft 
	segregations; Sharp change to - 
	3.29 - 3.54 m	Brown (7.5YR5/4-Moist); , 10YR53; Light medium clay; Moderate grade of structure, 5-10 mm, 
	Polyhedral; Strong consistence; Few (2 - 10 %), Calcareous, Coarse (6 - 20 mm), Concretions; 
	Morphological Notes
	KO1
	KO2
	K21
	K22
	K23
	KM1
	KM2
	KM3
	KM3
	KM3
	K31
	K32
	K33
	K33
	K34
	Observation Notes
	FREQUENT MICA THROUGH SAMPLE:                                                                                           
	Site Notes
	HARRY CREEK 1

	Project Name:	CAS
	Project Code:	CAS	Site ID:	NT89	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.4	6.8H	 0.04C
	0.4 - 0.8	7.3H	 0.014C
	0.8 - 1	8.1H	 0.015C
	1 - 1.18	8.1H	 0.021C
	1.18 - 1.33	8.8H	 0.043C
	1.33 - 1.41	9H	 0.019C
	1.41 - 1.51	9.1H	 0.027C
	1.51 - 1.66	9H	 0.02C
	1.91 - 2.21	9H	 0.027C
	2.21 - 2.57	9.1H	 0.025C
	2.57 - 2.62	9.2H	 0.025C
	2.62 - 2.7	9.2H	 0.049C
	2.73 - 2.99	9.3H	 0.077C
	2.99 - 3.24	9.3H	 0.076C
	3.29 - 3.54	9.4H	 0.08C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.4	 0.054B	 5	 13C	 25	 8	 38
	0.4 - 0.8	 0.041B
	0.8 - 1	 0.01C	 0.029B	 1	 8C	 30	 33	 23
	1 - 1.18	 0.02C	 6C	 35	 41	 13
	1.18 - 1.33	 1.5C	 0.026B	 1	 7C	 43	 39	 4
	1.33 - 1.41	 0.07C	 0.01B	 1	 33C	 43	 9	 10
	1.41 - 1.51	 0.1C	 2	 20C	 27	 29	 19
	1.51 - 1.66	 0.14C	 0.015B	 1	 27C	 21	 15	 30
	1.91 - 2.21	 0.15C	 0.018B	 1	 16C	 27	 21	 29
	2.21 - 2.57	 0.11C	 1	 21C	 27	 15	 31
	2.57 - 2.62	 0.81C	 0.01B	 1	 48C	 19	 5	 23
	2.62 - 2.7	 0.32C	 2	 21C	 22	 11	 40
	2.73 - 2.99	 2.1C	 2	 15C	 24	 13	 42
	2.99 - 3.24	 0.14C	 0.012B	 1	 13C	 27	 12	 43
	3.29 - 3.54	 0.64C	 4	 16C	 18	 14	 46
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.4
	0.4 - 0.8
	0.8 - 1
	1 - 1.18
	1.18 - 1.33
	1.33 - 1.41
	1.41 - 1.51
	1.51 - 1.66
	1.91 - 2.21
	2.21 - 2.57
	2.57 - 2.62

	Project Name:	CAS
	Project Code:	CAS	Site ID:	NT89	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	2.62 - 2.7
	2.73 - 2.99
	2.99 - 3.24
	3.29 - 3.54

	Project Name:	CAS
	Project Code:	CAS	Site ID:	NT89	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (NT)
	Laboratory Analyses Completed for this profile
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	7_NR	Total nitrogen (%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded