Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW116	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	333 metres
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6082775 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	541625  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Cza	Substrate Material:	Clay 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Valley flat	Slope Category:	No Data
	Slope:	3 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Partial, Minor (gully) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.21
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.12 m	Brown (7.5YR4/3-Moist); ; Silty clay loam; Weak grade of structure, 100-200 mm, Prismatic; 
	Earthy fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Common (1-5 per 100mm2)
	 Very fine (0.075-1mm) macropores, Moist; Moderately plastic; Moderately sticky; Field pH 5.5 
	(Raupach); Many, fine (1-2mm) roots; Gradual, Smooth change to - 
	A2	0.12 - 0.22 m	Brown (10YR5/3-Moist); Light grey (10YR7/2-Dry); Mottles, 0-2% , Distinct; Silty clay loam; Weak 
	grade of structure, 100-200 mm, Prismatic; Earthy fabric; Common (1-5 per 100mm2) Fine (1-
	2mm) macropores, Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Moist; 
	Moderately plastic; Moderately sticky; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm),
	 Soft segregations, weak, segregations;Field pH 6 (Raupach); Common, fine (1-2mm) roots; 
	Clear, Smooth change to - 
	B	0.22 - 0.8 m	Yellowish brown (10YR5/4-Moist); Mottles, 10-20% , Distinct; Mottles, 2-10% , Faint; Medium 
	clay; Moderate grade of structure, 2-5 mm, Polyhedral; Rough-ped fabric; Few (<1 per 100mm2) 
	Fine (1-2mm) macropores, Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moist; Very
	 plastic; Very sticky; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Soft 
	segregations, weak, segregations;Field pH 6 (Raupach); Common, fine (1-2mm) roots; 
	Morphological Notes
	A2	Weakly developed A2.                                                                                                          
	                                                                          
	Observation Notes
	Site Notes
	30M IN FENCE AT DRAINAGE LINE         

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW116	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW116	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile