Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW124	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Site Information
	Desc. By:	Chen, XY	Locality:
	Date Desc.:	15/07/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8327   1:25000	Rainfall:	No Data
	Northing/Long.:	6083250 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	535575  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Ou	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	8 % 	Aspect:	315 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dr3.41
	ASC Confidence:	Great Soil Group:	Soloth
	Confidence level not specified
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.12 m	Dark reddish grey (5YR4/2-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Common (1-5 per 100mm2) Fine
	 (1-2mm) macropores, Moist; Non-plastic; Slightly sticky; 0-2%, fine gravelly, 2-6mm, 
	subangular, dispersed, coarse fragments; Field pH 5 (Raupach); Common, fine (1-2mm) roots; 
	Clear, Irregular change to - 
	A2	0.12 - 0.45 m	Brown (7.5YR5/4-Moist); Very pale brown (10YR7/4-Dry); ; Fine sandy loam; Massive grade of 
	structure; Earthy fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Moist; Non-plastic; Slightly sticky; 0-2%, 
	fine gravelly, 2-6mm, subangular, dispersed, coarse fragments; Field pH 5 (Raupach); Common,
	 fine (1-2mm) roots; Gradual change to - 
	B	0.45 - 0.85 m	Yellowish red (5YR4/6-Moist); Mottles, 20-50% , Faint; Mottles, 2-10% , Faint; Fine sandy 
	medium clay; Moderate grade of structure, 2-5 mm, Granular; Rough-ped fabric; Moist; 
	Moderately plastic; Moderately sticky; 0-2%, fine gravelly, 2-6mm, subangular, dispersed, coarse
	 fragments; Field pH 5 (Raupach); Few, fine (1-2mm) roots; 
	Morphological Notes
	A1	Sandstone, siltstone pieces.                                                                                               
	                                                                             
	A2	Some disturbance indicated by buried log                                                                           
	                                                                                     
	B	Siltstone, phyllite pieces.                                                                                                     
	                                                                        
	Observation Notes
	Pit to 30cm, auger to 85cm.                                                                                                                                                               
	              
	Site Notes

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW124	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	WAGGA WAGGA SOIL LANDSCAPES             
	Project Code:	1000448	Site ID:	WW124	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (ACT)
	Laboratory Analyses Completed for this profile